(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PCM6140-Q1"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 53.34 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PCM6140-Q1"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PCM6140-Q1"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/pcm6140-q1.pdf?ts=1735826261657&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FPCM6140-Q1"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Automotive, quad-channel 768-kHz audio converter (ADC), 122-dB SNR, VQFN24"
				(at 53.34 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PCM6140QRGERQ1"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, CONVERTER, IC, ADC, AUDIO, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PCM6140-Q1_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "AVDD")
					(number "1")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "AREG")
					(number "2")
				)
				(pin power_out line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VREF")
					(number "3")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 2.54)
					(name "AVSS")
					(number "4")
				)
				(pin output line
					(at 38.1 -22.86 180)
					(length 2.54)
					(name "MICBIAS")
					(number "5")
				)
				(pin bidirectional line
					(at 38.1 0 180)
					(length 2.54)
					(name "IN1P_GPI1")
					(number "6")
				)
				(pin bidirectional line
					(at 38.1 -2.54 180)
					(length 2.54)
					(name "IN1M_GPO1")
					(number "7")
				)
				(pin bidirectional line
					(at 38.1 -5.08 180)
					(length 2.54)
					(name "IN2P_GPI2")
					(number "8")
				)
				(pin bidirectional line
					(at 38.1 -7.62 180)
					(length 2.54)
					(name "IN2M_GPO2")
					(number "9")
				)
				(pin bidirectional line
					(at 38.1 -10.16 180)
					(length 2.54)
					(name "IN3P_GPI3")
					(number "10")
				)
				(pin bidirectional line
					(at 38.1 -12.7 180)
					(length 2.54)
					(name "IN3M_GPO3")
					(number "11")
				)
				(pin bidirectional line
					(at 38.1 -15.24 180)
					(length 2.54)
					(name "IN4P_GPI4")
					(number "12")
				)
				(pin bidirectional line
					(at 38.1 -17.78 180)
					(length 2.54)
					(name "IN4M_GPO4")
					(number "13")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "SHDNZ")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "ADDR1_MISO")
					(number "15")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "ADDR0_SCLK")
					(number "16")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "SCL_MOSI")
					(number "17")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "SDA_SSZ")
					(number "18")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "IOVDD")
					(number "19")
				)
				(pin bidirectional line
					(at 38.1 -27.94 180)
					(length 2.54)
					(name "GPIO1")
					(number "20")
				)
				(pin output line
					(at 38.1 -33.02 180)
					(length 2.54)
					(name "SDOUT")
					(number "21")
				)
				(pin bidirectional line
					(at 38.1 -35.56 180)
					(length 2.54)
					(name "BCLK")
					(number "22")
				)
				(pin bidirectional line
					(at 38.1 -38.1 180)
					(length 2.54)
					(name "FSYNC")
					(number "23")
				)
				(pin power_out line
					(at 0 -10.16 0)
					(length 2.54)
					(name "DREG")
					(number "24")
				)
				(pin power_in line
					(at 0 -35.56 0)
					(length 2.54)
					(name "EP")
					(number "25")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(hide yes)
					(name "AVSS")
					(number "A1")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(hide yes)
					(name "AVSS")
					(number "A2")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(hide yes)
					(name "AVSS")
					(number "A3")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(hide yes)
					(name "AVSS")
					(number "A4")
				)
			)
			(embedded_fonts no)
		)
)
