(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PDQE30-Q48-S12-D"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PDQE30-Q48-S12-D"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PDQE30-Q48-S12-D"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.cui.com/product/resource/pdqe30-d.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Isolated Through Hole DC/DC Converter, ITE, 4:1, 30 W, 1 Output, 12 V, 2.5 A"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PDQE30-Q48-S12-D"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "CUI Inc"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "THT, PMIC, IC, DC-DC, CONVERTER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PDQE30-Q48-S12-D_1_1"
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "CTRL")
					(number "1")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{IN}")
					(number "3")
				)
				(pin power_out line
					(at 20.32 0 180)
					(length 2.54)
					(name "V_{O}")
					(number "4")
				)
				(pin passive line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "TRIM")
					(number "5")
				)
				(pin power_out line
					(at 20.32 -15.24 180)
					(length 2.54)
					(name "0V")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
