(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SSQE48T07120-NABNG"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 44.45 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SSQE48T07120-NABNG"
				(at 44.45 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SSQE48T07120-NABNG"
				(at 44.45 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.belfuse.com/resources/datasheets/powersolutions/ds-bps-ssqe48t07120-series.pdf"
				(at 44.45 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DC/DC converter"
				(at 44.45 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SSQE48T07120-NABNG"
				(at 44.45 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Bel Fuse"
				(at 44.45 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 44.45 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 44.45 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "THT, PMIC, IC, DC-DC, CONVERTER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SSQE48T07120-NABNG_0_0"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN+")
					(number "1")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "ON/OFF")
					(number "2")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "VIN-")
					(number "3")
				)
				(pin power_out line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "VOUT-")
					(number "4")
				)
				(pin passive line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "SENSE-")
					(number "5")
				)
				(pin passive line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "TRIM")
					(number "6")
				)
				(pin passive line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "SENSE+")
					(number "7")
				)
				(pin power_out line
					(at 25.4 0 180)
					(length 2.54)
					(name "VOUT+")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
