(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS3840PL30DBVR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS3840PL30DBVR"
				(at 38.1 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS3840PL30DBVR"
				(at 38.1 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps3840.pdf?HQS=dis-mous-null-mousermode-dsf-pf-null-wwe&DCM=yes&ref_url=https%3A%2F%2Fwww.mouser.com%2F&distId=26"
				(at 38.1 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Voltage supervisor"
				(at 38.1 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 38.1 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS3840PL30DBVR"
				(at 38.1 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 38.1 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, CONTROLLER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "DBV0005A_N DBV0005A_M DBV0005A_L"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS3840PL30DBVR_1_1"
				(pin output line
					(at 17.78 0 180)
					(length 2.54)
					(name "~{RESET}")
					(number "1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "2")
				)
				(pin power_in line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{MR}")
					(number "4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "CT")
					(number "5")
				)
			)
			(embedded_fonts no)
		)
)
