(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS51200DRCT"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS51200DRCT"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS51200DRCT"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps51200.pdf?ts=1685420125657"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Fixed LDO Voltage Regulator, 2.375 V to 3.5 V, 0.8 V Dropout, 1.25 V / 3 A out, VSON-10"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS51200DRCT"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "*VSON?10?1EP?3x3mm?P0.5mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS51200DRCT_0_1"
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "REFIN")
					(number "1")
				)
				(pin power_in line
					(at 0 -11.43 0)
					(length 2.54)
					(name "VLDOIN")
					(number "2")
				)
				(pin power_out line
					(at 20.32 0 180)
					(length 2.54)
					(name "VO")
					(number "3")
				)
				(pin passive line
					(at 20.32 -11.43 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "4")
				)
				(pin input line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "VOSNS")
					(number "5")
				)
				(pin power_out line
					(at 20.32 -8.89 180)
					(length 2.54)
					(name "REFOUT")
					(number "6")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "EN")
					(number "7")
				)
				(pin power_in line
					(at 20.32 -11.43 180)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin open_collector line
					(at 0 -2.54 0)
					(length 2.54)
					(name "PGOOD")
					(number "9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "10")
				)
				(pin passive line
					(at 20.32 -11.43 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "11")
				)
			)
			(embedded_fonts no)
		)
)
