(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS65086100"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 63.5 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS65086100"
				(at 63.5 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS65086100"
				(at 63.5 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps650861.pdf"
				(at 63.5 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Programmable Multirail PMU"
				(at 63.5 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS65086100"
				(at 63.5 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 63.5 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 63.5 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 63.5 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, MANAGEMENT, BATTERY"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS65086100_1_1"
				(pin power_in line
					(at 30.48 -34.29 180)
					(length 2.54)
					(name "FBGND2")
					(number "1")
				)
				(pin input line
					(at 30.48 -29.21 180)
					(length 2.54)
					(name "FBVOUT2")
					(number "2")
				)
				(pin output line
					(at 30.48 -21.59 180)
					(length 2.54)
					(name "DRVH2")
					(number "3")
				)
				(pin input line
					(at 30.48 -24.13 180)
					(length 2.54)
					(name "SW2")
					(number "4")
				)
				(pin input line
					(at 30.48 -19.05 180)
					(length 2.54)
					(name "BOOT2")
					(number "5")
				)
				(pin power_in line
					(at 30.48 -31.75 180)
					(length 2.54)
					(name "PGNDSNS2")
					(number "6")
				)
				(pin output line
					(at 30.48 -26.67 180)
					(length 2.54)
					(name "DRVL2")
					(number "7")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "DRV5V_2_A1")
					(number "8")
				)
				(pin power_out line
					(at 0 -73.66 0)
					(length 2.54)
					(name "LDOA1")
					(number "9")
				)
				(pin power_out line
					(at 30.48 -40.64 180)
					(length 2.54)
					(name "LX3")
					(number "10")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "PVIN3")
					(number "11")
				)
				(pin input line
					(at 30.48 -43.18 180)
					(length 2.54)
					(name "FB3")
					(number "12")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "CTL1")
					(number "13")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "CTL6_SLPENB2")
					(number "14")
				)
				(pin output line
					(at 0 -53.34 0)
					(length 2.54)
					(name "IRQB")
					(number "15")
				)
				(pin output line
					(at 0 -58.42 0)
					(length 2.54)
					(name "GPO1")
					(number "16")
				)
				(pin power_out line
					(at 30.48 -81.28 180)
					(length 2.54)
					(name "SWB1")
					(number "17")
				)
				(pin power_in line
					(at 0 -26.67 0)
					(length 2.54)
					(name "PVINSWB1_B2")
					(number "18")
				)
				(pin power_out line
					(at 30.48 -83.82 180)
					(length 2.54)
					(name "SWB2")
					(number "19")
				)
				(pin power_out line
					(at 30.48 -53.34 180)
					(length 2.54)
					(name "LX5")
					(number "20")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "PVIN5")
					(number "21")
				)
				(pin input line
					(at 30.48 -55.88 180)
					(length 2.54)
					(name "FB5")
					(number "22")
				)
				(pin input line
					(at 30.48 -49.53 180)
					(length 2.54)
					(name "FB4")
					(number "23")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "PVIN4")
					(number "24")
				)
				(pin power_out line
					(at 30.48 -46.99 180)
					(length 2.54)
					(name "LX4")
					(number "25")
				)
				(pin output line
					(at 0 -60.96 0)
					(length 2.54)
					(name "GPO2")
					(number "26")
				)
				(pin output line
					(at 0 -55.88 0)
					(length 2.54)
					(name "GPO3")
					(number "27")
				)
				(pin output line
					(at 0 -63.5 0)
					(length 2.54)
					(name "GPO4")
					(number "28")
				)
				(pin input line
					(at 30.48 -10.16 180)
					(length 2.54)
					(name "FBVOUT1")
					(number "29")
				)
				(pin input line
					(at 30.48 -15.24 180)
					(length 2.54)
					(name "ILIM1")
					(number "30")
				)
				(pin power_out line
					(at 30.48 -78.74 180)
					(length 2.54)
					(name "SWA1")
					(number "31")
				)
				(pin power_in line
					(at 0 -24.13 0)
					(length 2.54)
					(name "PVINSWA1")
					(number "32")
				)
				(pin output line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "DRVH1")
					(number "33")
				)
				(pin input line
					(at 30.48 -5.08 180)
					(length 2.54)
					(name "SW1")
					(number "34")
				)
				(pin input line
					(at 30.48 0 180)
					(length 2.54)
					(name "BOOT1")
					(number "35")
				)
				(pin power_in line
					(at 30.48 -12.7 180)
					(length 2.54)
					(name "PGNDSNS1")
					(number "36")
				)
				(pin output line
					(at 30.48 -7.62 180)
					(length 2.54)
					(name "DRVL1")
					(number "37")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DRV5V_1_6")
					(number "38")
				)
				(pin output line
					(at 30.48 -67.31 180)
					(length 2.54)
					(name "DRVL6")
					(number "39")
				)
				(pin power_in line
					(at 30.48 -72.39 180)
					(length 2.54)
					(name "PGNDSNS6")
					(number "40")
				)
				(pin input line
					(at 30.48 -59.69 180)
					(length 2.54)
					(name "BOOT6")
					(number "41")
				)
				(pin input line
					(at 30.48 -64.77 180)
					(length 2.54)
					(name "SW6")
					(number "42")
				)
				(pin output line
					(at 30.48 -62.23 180)
					(length 2.54)
					(name "DRVH6")
					(number "43")
				)
				(pin input line
					(at 30.48 -69.85 180)
					(length 2.54)
					(name "FBVOUT6")
					(number "44")
				)
				(pin input line
					(at 30.48 -74.93 180)
					(length 2.54)
					(name "ILIM6")
					(number "45")
				)
				(pin power_in line
					(at 0 -8.89 0)
					(length 2.54)
					(name "PVINVTT")
					(number "46")
				)
				(pin power_out line
					(at 0 -67.31 0)
					(length 2.54)
					(name "VTT")
					(number "47")
				)
				(pin input line
					(at 0 -69.85 0)
					(length 2.54)
					(name "VTTFB")
					(number "48")
				)
				(pin power_out line
					(at 0 -78.74 0)
					(length 2.54)
					(name "LDOA3")
					(number "49")
				)
				(pin power_in line
					(at 0 -21.59 0)
					(length 2.54)
					(name "PVINLDOA2_A3")
					(number "50")
				)
				(pin power_out line
					(at 0 -76.2 0)
					(length 2.54)
					(name "LDOA2")
					(number "51")
				)
				(pin power_in line
					(at 30.48 -90.17 180)
					(length 2.54)
					(name "AGND")
					(number "52")
				)
				(pin output line
					(at 30.48 -87.63 180)
					(length 2.54)
					(name "VREF")
					(number "53")
				)
				(pin output line
					(at 0 -85.09 0)
					(length 2.54)
					(name "LDO3P3")
					(number "54")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "VSYS")
					(number "55")
				)
				(pin output line
					(at 0 -82.55 0)
					(length 2.54)
					(name "LDO5P0")
					(number "56")
				)
				(pin input line
					(at 0 -87.63 0)
					(length 2.54)
					(name "V5ANA")
					(number "57")
				)
				(pin input line
					(at 0 -46.99 0)
					(length 2.54)
					(name "CLK")
					(number "58")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 2.54)
					(name "DATA")
					(number "59")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 2.54)
					(name "CTL2")
					(number "60")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "CTL3_SLPENB1")
					(number "61")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "CTL4")
					(number "62")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "CTL5")
					(number "63")
				)
				(pin input line
					(at 30.48 -36.83 180)
					(length 2.54)
					(name "ILIM2")
					(number "64")
				)
				(pin power_in line
					(at 30.48 -92.71 180)
					(length 2.54)
					(name "GND")
					(number "65")
				)
			)
			(embedded_fonts no)
		)
)
