(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS65150_HTSSOP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 40.64 12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS65150_HTSSOP"
				(at 40.64 7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS65150_HTSSOP"
				(at 40.64 5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps65150.pdf?ts=1698145244786&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FTPS65150%252Fpart-details%252FTPS65150PWP"
				(at 40.64 2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Universal LCD bias Power Supply with integrated VCOM Buffer"
				(at 40.64 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 40.64 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS65150PWP"
				(at 40.64 10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 40.64 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 40.64 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "BOOST, CONVERTER, CONTROLLER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS65150_HTSSOP_1_1"
				(pin passive line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "FB")
					(number "1")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "DLY1")
					(number "2")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "DLY2")
					(number "3")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "4")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 2.54)
					(name "SW")
					(number "5")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 2.54)
					(name "SW")
					(number "6")
				)
				(pin power_in line
					(at 0 -48.26 0)
					(length 2.54)
					(name "PGND")
					(number "7")
				)
				(pin power_in line
					(at 0 -48.26 0)
					(length 2.54)
					(name "PGND")
					(number "8")
				)
				(pin passive line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "SUP")
					(number "9")
				)
				(pin power_out line
					(at 25.4 -50.8 180)
					(length 2.54)
					(name "VCOM")
					(number "10")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(name "IN")
					(number "11")
				)
				(pin passive line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "FBP")
					(number "12")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "CTRL")
					(number "13")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "ADJ")
					(number "14")
				)
				(pin power_out line
					(at 25.4 -40.64 180)
					(length 2.54)
					(name "VGH")
					(number "15")
				)
				(pin passive line
					(at 25.4 -22.86 180)
					(length 2.54)
					(name "CPI")
					(number "16")
				)
				(pin passive line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "DRVP")
					(number "17")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DRVN")
					(number "18")
				)
				(pin power_in line
					(at 0 -50.8 0)
					(length 2.54)
					(name "AGND")
					(number "19")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "REF")
					(number "20")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "FBN")
					(number "21")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "COMP")
					(number "22")
				)
				(pin passive line
					(at 25.4 -25.4 180)
					(length 2.54)
					(name "GD")
					(number "23")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "FDLY")
					(number "24")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(name "EP")
					(number "25")
				)
			)
			(embedded_fonts no)
		)
)
