(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS658621A"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 50.546 -11.938 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS658621A"
				(at 50.8 -16.256 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS658621A"
				(at 50.8 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.alldatasheet.com/datasheet-pdf/view/355213/TI/TPS658621A.html"
				(at 50.8 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Fully integrated solution for handheld devices, integrating charge management, multiple regulated power supplies, system management and display functions. I2C interface enables control of a wide range of subsystem parameters."
				(at 50.8 -29.718 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS658621A"
				(at 50.8 -14.224 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 50.8 -23.622 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 50.8 -27.178 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 50.8 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "BGA, DC-DC, LDO, SMT, BUCK, IC, PMIC, CHARGER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS658621A_1_0"
				(pin bidirectional line
					(at 38.1 0 180)
					(length 3.81)
					(name "~{HOT_RST}")
					(number "A2")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 3.81)
					(name "TNOPOWER")
					(number "A3")
				)
				(pin input line
					(at 0 -92.71 0)
					(length 3.81)
					(name "AGND3")
					(number "A4")
				)
				(pin output line
					(at 38.1 -77.47 180)
					(length 3.81)
					(name "SM1PG")
					(number "A5")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "RESUME")
					(number "B2")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "LDO4EN")
					(number "B3")
				)
				(pin output line
					(at 38.1 -74.93 180)
					(length 3.81)
					(name "SM0PG")
					(number "B4")
				)
				(pin input line
					(at 0 -92.71 0)
					(length 3.81)
					(hide yes)
					(name "AGND3")
					(number "B5")
				)
				(pin input line
					(at 0 -92.71 0)
					(length 3.81)
					(hide yes)
					(name "AGND3")
					(number "C5")
				)
				(pin output line
					(at 38.1 -17.78 180)
					(length 3.81)
					(name "OUT32K")
					(number "C7")
				)
				(pin output line
					(at 38.1 -22.86 180)
					(length 3.81)
					(name "~{NORTC}")
					(number "D4")
				)
				(pin bidirectional line
					(at 38.1 -87.63 180)
					(length 3.81)
					(name "DGND2DT")
					(number "D6")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "V32K")
					(number "D7")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "SYNCEN")
					(number "E10")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "SM1EN")
					(number "E11")
				)
				(pin output line
					(at 38.1 -57.15 180)
					(length 3.81)
					(name "DIG_PWM2")
					(number "F4")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 3.81)
					(name "SM0EN")
					(number "F10")
				)
				(pin input line
					(at 38.1 -67.31 180)
					(length 3.81)
					(name "SCLK")
					(number "H4")
				)
				(pin bidirectional line
					(at 38.1 -64.77 180)
					(length 3.81)
					(name "SDAT")
					(number "J2")
				)
				(pin input line
					(at 0 -67.31 0)
					(length 3.81)
					(name "PSCLK")
					(number "J3")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 3.81)
					(name "PSDAT")
					(number "J4")
				)
				(pin input line
					(at 0 -87.63 0)
					(length 3.81)
					(name "AGND1")
					(number "J10")
				)
				(pin output line
					(at 38.1 -29.21 180)
					(length 3.81)
					(name "V2V2")
					(number "J11")
				)
				(pin output line
					(at 38.1 -31.75 180)
					(length 3.81)
					(name "VREF1V25")
					(number "J12")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "ADC_REF")
					(number "K3")
				)
				(pin input line
					(at 0 -90.17 0)
					(length 3.81)
					(name "AGND2")
					(number "K4")
				)
				(pin input line
					(at 38.1 -90.17 180)
					(length 3.81)
					(name "DGND1")
					(number "K6")
				)
				(pin output line
					(at 38.1 -39.37 180)
					(length 3.81)
					(name "RED2")
					(number "K8")
				)
				(pin input line
					(at 38.1 -59.69 180)
					(length 3.81)
					(name "PWM")
					(number "K9")
				)
				(pin output line
					(at 38.1 -26.67 180)
					(length 3.81)
					(name "AVDD6")
					(number "K13")
				)
				(pin output line
					(at 38.1 -80.01 180)
					(length 3.81)
					(name "LDO4PG")
					(number "L1")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 3.81)
					(name "ANLG2")
					(number "L3")
				)
				(pin output line
					(at 38.1 -44.45 180)
					(length 3.81)
					(name "GREEN2")
					(number "L8")
				)
				(pin output line
					(at 38.1 -36.83 180)
					(length 3.81)
					(name "RED1")
					(number "L9")
				)
				(pin output line
					(at 38.1 -15.24 180)
					(length 3.81)
					(name "~{INT}")
					(number "L10")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 3.81)
					(name "ANLG1")
					(number "M1")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 3.81)
					(name "ANLG3")
					(number "M2")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 3.81)
					(name "GPIO1")
					(number "M3")
				)
				(pin bidirectional line
					(at 0 -77.47 0)
					(length 3.81)
					(name "GPIO3")
					(number "M4")
				)
				(pin input line
					(at 0 -54.61 0)
					(length 3.81)
					(name "XTAL1")
					(number "M6")
				)
				(pin output line
					(at 38.1 -49.53 180)
					(length 3.81)
					(name "BLUE2")
					(number "M8")
				)
				(pin output line
					(at 38.1 -41.91 180)
					(length 3.81)
					(name "GREEN1")
					(number "M9")
				)
				(pin output line
					(at 38.1 -20.32 180)
					(length 3.81)
					(name "~{NOPOWER}")
					(number "M11")
				)
				(pin input line
					(at 0 -82.55 0)
					(length 3.81)
					(name "COMP")
					(number "N1")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "N2")
				)
				(pin bidirectional line
					(at 0 -74.93 0)
					(length 3.81)
					(name "GPIO2")
					(number "N3")
				)
				(pin bidirectional line
					(at 0 -80.01 0)
					(length 3.81)
					(name "GPIO4")
					(number "N4")
				)
				(pin input line
					(at 0 -57.15 0)
					(length 3.81)
					(name "XTAL2")
					(number "N6")
				)
				(pin output line
					(at 38.1 -46.99 180)
					(length 3.81)
					(name "BLUE1")
					(number "N9")
				)
				(pin output line
					(at 38.1 -52.07 180)
					(length 3.81)
					(name "LED_PWM")
					(number "N10")
				)
				(pin output line
					(at 38.1 -54.61 180)
					(length 3.81)
					(name "DIG_PWM")
					(number "N11")
				)
			)
			(symbol "TPS658621A_1_1"
				(text "RTC\nOSCILLATOR"
					(at 13.716 -55.88 0)
				)
				(text "ADC"
					(at 14.478 -41.656 0)
				)
				(text "REFERENCE\nSYSTEM"
					(at 18.796 -28.702 0)
				)
				(text "I2C INTERFACE"
					(at 18.796 -66.04 0)
				)
				(text "INPUT/OUTPUT"
					(at 18.796 -77.216 0)
				)
				(text "ANALOG\nDIGITAL\nGND"
					(at 18.796 -89.408 0)
				)
				(text "EXTERNAL SYSTEM RESET\nCLOCK OUTPUTS\nADJUSTABLE LEVEL"
					(at 19.05 -16.764 0)
				)
				(text "SEQUENCING\nCONTROL\nINPUTS"
					(at 19.304 -5.334 0)
				)
				(text "DRIVERS"
					(at 22.352 -49.276 900)
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(name "HSK")
					(number "D5")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "D8")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "D9")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "D10")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "E4")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "E5")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "E6")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "E7")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "E8")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "E9")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "F5")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "F6")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "F7")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "F8")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "F9")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "G5")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "G6")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "G7")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "G8")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "G9")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "H5")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "H6")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "H7")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "H8")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "H9")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "J5")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "J6")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "J7")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "J8")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "J9")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "K5")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "K7")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "K10")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "L4")
				)
				(pin output line
					(at 38.1 -92.71 180)
					(length 3.81)
					(hide yes)
					(name "HSK")
					(number "L5")
				)
			)
			(symbol "TPS658621A_2_0"
				(pin input line
					(at 0 -58.42 0)
					(length 3.81)
					(name "VIN_SM0")
					(number "A1")
				)
				(pin input line
					(at 0 -26.67 0)
					(length 3.81)
					(name "VIN_LDO23")
					(number "A6")
				)
				(pin output line
					(at 38.1 -35.56 180)
					(length 3.81)
					(name "LDO5")
					(number "A7")
				)
				(pin input line
					(at 38.1 -93.98 180)
					(length 3.81)
					(name "PGND2")
					(number "A8")
				)
				(pin output line
					(at 38.1 -73.66 180)
					(length 3.81)
					(name "L2")
					(number "A9")
				)
				(pin input line
					(at 0 -73.66 0)
					(length 3.81)
					(name "VIN_SM2")
					(number "A10")
				)
				(pin output line
					(at 38.1 0 180)
					(length 3.81)
					(name "SYS")
					(number "A11")
				)
				(pin output line
					(at 38.1 0 180)
					(length 3.81)
					(hide yes)
					(name "SYS")
					(number "A12")
				)
				(pin output line
					(at 38.1 0 180)
					(length 3.81)
					(hide yes)
					(name "SYS")
					(number "A13")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 3.81)
					(hide yes)
					(name "VIN_SM0")
					(number "B1")
				)
				(pin output line
					(at 38.1 -29.21 180)
					(length 3.81)
					(name "LDO3")
					(number "B6")
				)
				(pin output line
					(at 38.1 -26.67 180)
					(length 3.81)
					(name "LDO2")
					(number "B7")
				)
				(pin input line
					(at 38.1 -93.98 180)
					(length 3.81)
					(hide yes)
					(name "PGND2")
					(number "B8")
				)
				(pin output line
					(at 38.1 -73.66 180)
					(length 3.81)
					(hide yes)
					(name "L2")
					(number "B9")
				)
				(pin input line
					(at 0 -73.66 0)
					(length 3.81)
					(hide yes)
					(name "VIN_SM2")
					(number "B10")
				)
				(pin output line
					(at 38.1 0 180)
					(length 3.81)
					(hide yes)
					(name "SYS")
					(number "B11")
				)
				(pin output line
					(at 38.1 0 180)
					(length 3.81)
					(hide yes)
					(name "SYS")
					(number "B12")
				)
				(pin output line
					(at 38.1 0 180)
					(length 3.81)
					(hide yes)
					(name "SYS")
					(number "B13")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 3.81)
					(hide yes)
					(name "VIN_SM0")
					(number "C1")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 3.81)
					(hide yes)
					(name "VIN_SM0")
					(number "C2")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 3.81)
					(hide yes)
					(name "VIN_SM0")
					(number "C3")
				)
				(pin input line
					(at 38.1 -60.96 180)
					(length 3.81)
					(name "SM0")
					(number "C4")
				)
				(pin input line
					(at 38.1 -68.58 180)
					(length 3.81)
					(name "SM1")
					(number "C6")
				)
				(pin input line
					(at 38.1 -93.98 180)
					(length 3.81)
					(hide yes)
					(name "PGND2")
					(number "C8")
				)
				(pin output line
					(at 38.1 -73.66 180)
					(length 3.81)
					(hide yes)
					(name "L2")
					(number "C9")
				)
				(pin input line
					(at 0 -73.66 0)
					(length 3.81)
					(hide yes)
					(name "VIN_SM2")
					(number "C10")
				)
				(pin output line
					(at 38.1 0 180)
					(length 3.81)
					(hide yes)
					(name "SYS")
					(number "C11")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "AC")
					(number "C12")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "AC")
					(number "C13")
				)
				(pin output line
					(at 38.1 -58.42 180)
					(length 3.81)
					(name "L0")
					(number "D1")
				)
				(pin output line
					(at 38.1 -58.42 180)
					(length 3.81)
					(hide yes)
					(name "L0")
					(number "D2")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 3.81)
					(hide yes)
					(name "VIN_SM0")
					(number "D3")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "AC")
					(number "D11")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "AC")
					(number "D12")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "AC")
					(number "D13")
				)
				(pin input line
					(at 0 -93.98 0)
					(length 3.81)
					(name "PGND0")
					(number "E1")
				)
				(pin input line
					(at 0 -93.98 0)
					(length 3.81)
					(hide yes)
					(name "PGND0")
					(number "E2")
				)
				(pin input line
					(at 0 -93.98 0)
					(length 3.81)
					(hide yes)
					(name "PGND0")
					(number "E3")
				)
				(pin input line
					(at 38.1 -76.2 180)
					(length 3.81)
					(name "SM2")
					(number "E12")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 3.81)
					(name "USB")
					(number "E13")
				)
				(pin input line
					(at 0 -96.52 0)
					(length 3.81)
					(name "PGND1")
					(number "F1")
				)
				(pin input line
					(at 0 -96.52 0)
					(length 3.81)
					(hide yes)
					(name "PGND1")
					(number "F2")
				)
				(pin input line
					(at 0 -96.52 0)
					(length 3.81)
					(hide yes)
					(name "PGND1")
					(number "F3")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 3.81)
					(hide yes)
					(name "USB")
					(number "F11")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 3.81)
					(hide yes)
					(name "USB")
					(number "F12")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 3.81)
					(hide yes)
					(name "USB")
					(number "F13")
				)
				(pin input line
					(at 38.1 -66.04 180)
					(length 3.81)
					(name "L1")
					(number "G1")
				)
				(pin input line
					(at 38.1 -66.04 180)
					(length 3.81)
					(hide yes)
					(name "L1")
					(number "G2")
				)
				(pin input line
					(at 0 -66.04 0)
					(length 3.81)
					(name "VIN_SM1")
					(number "G3")
				)
				(pin output line
					(at 38.1 -39.37 180)
					(length 3.81)
					(name "LDO6")
					(number "G4")
				)
				(pin bidirectional line
					(at 38.1 -3.81 180)
					(length 3.81)
					(name "BAT")
					(number "G10")
				)
				(pin bidirectional line
					(at 38.1 -3.81 180)
					(length 3.81)
					(hide yes)
					(name "BAT")
					(number "G11")
				)
				(pin bidirectional line
					(at 38.1 -3.81 180)
					(length 3.81)
					(hide yes)
					(name "BAT")
					(number "G12")
				)
				(pin bidirectional line
					(at 38.1 -3.81 180)
					(length 3.81)
					(hide yes)
					(name "BAT")
					(number "G13")
				)
				(pin input line
					(at 0 -66.04 0)
					(length 3.81)
					(hide yes)
					(name "VIN_SM1")
					(number "H1")
				)
				(pin input line
					(at 0 -66.04 0)
					(length 3.81)
					(hide yes)
					(name "VIN_SM1")
					(number "H2")
				)
				(pin input line
					(at 0 -66.04 0)
					(length 3.81)
					(hide yes)
					(name "VIN_SM1")
					(number "H3")
				)
				(pin output line
					(at 38.1 -53.34 180)
					(length 3.81)
					(name "RTC_OUT")
					(number "H10")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "VIN_CHG")
					(number "H11")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "VIN_CHG")
					(number "H12")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "VIN_CHG")
					(number "H13")
				)
				(pin input line
					(at 0 -39.37 0)
					(length 3.81)
					(name "VIN_LDO678")
					(number "J1")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "TS")
					(number "J13")
				)
				(pin output line
					(at 38.1 -44.45 180)
					(length 3.81)
					(name "LDO8")
					(number "K1")
				)
				(pin output line
					(at 38.1 -41.91 180)
					(length 3.81)
					(name "LDO7")
					(number "K2")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "ISET")
					(number "K11")
				)
				(pin bidirectional line
					(at 38.1 -88.9 180)
					(length 3.81)
					(name "SM3IG")
					(number "K12")
				)
				(pin output line
					(at 38.1 -15.24 180)
					(length 3.81)
					(name "CHG_STAT")
					(number "L2")
				)
				(pin output line
					(at 38.1 -22.86 180)
					(length 3.81)
					(name "LDO1")
					(number "L6")
				)
				(pin output line
					(at 38.1 -33.02 180)
					(length 3.81)
					(name "LDO4")
					(number "L7")
				)
				(pin input line
					(at 0 -82.55 0)
					(length 3.81)
					(name "SM3")
					(number "L11")
				)
				(pin input line
					(at 38.1 -96.52 180)
					(length 3.81)
					(name "PGND3")
					(number "L12")
				)
				(pin input line
					(at 38.1 -96.52 180)
					(length 3.81)
					(hide yes)
					(name "PGND3")
					(number "L13")
				)
				(pin output line
					(at 38.1 -20.32 180)
					(length 3.81)
					(name "LDO0")
					(number "M5")
				)
				(pin output line
					(at 38.1 -48.26 180)
					(length 3.81)
					(name "LDO9")
					(number "M7")
				)
				(pin output line
					(at 38.1 -10.16 180)
					(length 3.81)
					(name "VTSBIAS")
					(number "M10")
				)
				(pin input line
					(at 0 -86.36 0)
					(length 3.81)
					(name "SM3_SW")
					(number "M12")
				)
				(pin output line
					(at 38.1 -81.28 180)
					(length 3.81)
					(name "L3")
					(number "M13")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 3.81)
					(name "VIN_LDO01")
					(number "N5")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 3.81)
					(name "VIN_LDO4")
					(number "N7")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 3.81)
					(name "VIN_LDO9")
					(number "N8")
				)
				(pin input line
					(at 38.1 -85.09 180)
					(length 3.81)
					(name "FB3")
					(number "N12")
				)
				(pin output line
					(at 38.1 -81.28 180)
					(length 3.81)
					(hide yes)
					(name "L3")
					(number "N13")
				)
			)
			(symbol "TPS658621A_2_1"
				(text "CHARGER"
					(at 18.796 -12.446 0)
				)
				(text "LINEAR\nREGULATORS"
					(at 18.796 -36.83 0)
				)
				(text "DC/DC\nCONVERTERS"
					(at 18.796 -67.564 0)
				)
				(text "SYSTEM\nPOWER\nPATH"
					(at 19.05 -1.27 0)
				)
				(text "SM3\nBOOST CONVERTER"
					(at 19.05 -85.344 0)
				)
				(text "DC/DC\nGND"
					(at 19.05 -94.996 0)
				)
			)
			(embedded_fonts no)
		)
)
