(footprint "TSSOP-44-1EP_W6.1mm_P0.635mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Based on: https://www.ti.com/lit/ds/symlink/tps7h4013-sep.pdf")
	(property "Reference" "REF**"
		(at -4.8 -7.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "TSSOP-44-1EP_W6.1mm_P0.635mm"
		(at -7.38 8.89 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0.025 -0.003 0)
		(layer "F.Fab")
	)
	(property "Description" ""
		(at 0.025 -0.003 0)
		(layer "F.Fab")
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -7.38 10.09 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -7.38 11.29 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -7.38 12.49 0)
		(layer "F.Fab")
	)
	(fp_text user ""
		(at 0.025 -0.003 0)
		(layer "User.5")
	)
	(fp_text user ""
		(at 0.025 -0.003 0)
		(layer "User.9")
	)
	(pad "" smd roundrect
		(at 0 0 90)
		(size 9.24 3.54)
		(layers "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "1" smd roundrect
		(at -3.75 -6.67 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "2" smd roundrect
		(at -3.75 -6.03 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "3" smd roundrect
		(at -3.75 -5.4 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "4" smd roundrect
		(at -3.75 -4.76 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "5" smd roundrect
		(at -3.75 -4.13 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "6" smd roundrect
		(at -3.75 -3.49 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "7" smd roundrect
		(at -3.75 -2.86 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "8" smd roundrect
		(at -3.75 -2.22 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "9" smd roundrect
		(at -3.75 -1.59 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "10" smd roundrect
		(at -3.75 -0.95 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "11" smd roundrect
		(at -3.75 -0.32 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "12" smd roundrect
		(at -3.75 0.32 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "13" smd roundrect
		(at -3.75 0.95 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "14" smd roundrect
		(at -3.75 1.59 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "15" smd roundrect
		(at -3.75 2.22 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "16" smd roundrect
		(at -3.75 2.86 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "17" smd roundrect
		(at -3.75 3.49 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "18" smd roundrect
		(at -3.75 4.13 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "19" smd roundrect
		(at -3.75 4.76 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "20" smd roundrect
		(at -3.75 5.4 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "21" smd roundrect
		(at -3.75 6.03 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "22" smd roundrect
		(at -3.75 6.67 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "23" smd roundrect
		(at 3.75 6.67 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "24" smd roundrect
		(at 3.75 6.03 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "25" smd roundrect
		(at 3.75 5.4 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "26" smd roundrect
		(at 3.75 4.76 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "27" smd roundrect
		(at 3.75 4.13 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "28" smd roundrect
		(at 3.75 3.49 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "29" smd roundrect
		(at 3.75 2.86 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "30" smd roundrect
		(at 3.75 2.22 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "31" smd roundrect
		(at 3.75 1.59 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "32" smd roundrect
		(at 3.75 0.95 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "33" smd roundrect
		(at 3.75 0.32 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "34" smd roundrect
		(at 3.75 -0.32 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "35" smd roundrect
		(at 3.75 -0.95 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "36" smd roundrect
		(at 3.75 -1.59 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "37" smd roundrect
		(at 3.75 -2.22 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "38" smd roundrect
		(at 3.75 -2.86 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "39" smd roundrect
		(at 3.75 -3.49 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "40" smd roundrect
		(at 3.75 -4.13 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "41" smd roundrect
		(at 3.75 -4.76 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "42" smd roundrect
		(at 3.75 -5.4 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "43" smd roundrect
		(at 3.75 -6.03 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "44" smd roundrect
		(at 3.75 -6.67 90)
		(size 0.4 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "45" smd roundrect
		(at 0 0 90)
		(size 14 5.2)
		(layers "F.Cu")
		(roundrect_rratio 0.05)
	)
	(embedded_fonts no)
	(model "antmicro_tps7h4012mddwtsep.glb"
		(offset
			(xyz 0.025 0.003 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
