(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS7H4012MDDWTSEP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Value" "TPS7H4012MDDWTSEP"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS7H4012MDDWTSEP"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps7h4013-sep.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Radiation Hardened Synchronous Buck Converter, Vin 4.5V to 14V, 3A"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS7H4012MDDWTSEP"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, No-RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS7H4012MDDWTSEP_1_1"
				(pin power_in line
					(at 0 -30.48 0)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "2")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "EN")
					(number "3")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "RT")
					(number "4")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VIN")
					(number "5")
				)
				(pin output line
					(at 24.13 -25.4 180)
					(length 2.54)
					(name "LDOCAP")
					(number "6")
				)
				(pin no_connect line
					(at 21.59 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "NC2")
					(number "7")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "SYNC1")
					(number "8")
				)
				(pin no_connect line
					(at 21.59 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "NC2")
					(number "9")
				)
				(pin passive line
					(at 24.13 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "NC1")
					(number "10")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "PVIN")
					(number "11")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "PVIN")
					(number "12")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "PVIN")
					(number "13")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "PVIN")
					(number "14")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "PVIN")
					(number "15")
				)
				(pin power_in line
					(at 24.13 -30.48 180)
					(length 2.54)
					(name "PGND")
					(number "16")
				)
				(pin passive line
					(at 24.13 -30.48 180)
					(length 2.54)
					(hide yes)
					(name "PGND")
					(number "17")
				)
				(pin passive line
					(at 24.13 -30.48 180)
					(length 2.54)
					(hide yes)
					(name "PGND")
					(number "18")
				)
				(pin passive line
					(at 24.13 -30.48 180)
					(length 2.54)
					(hide yes)
					(name "PGND")
					(number "19")
				)
				(pin passive line
					(at 24.13 -30.48 180)
					(length 2.54)
					(hide yes)
					(name "PGND")
					(number "20")
				)
				(pin passive line
					(at 24.13 -30.48 180)
					(length 2.54)
					(hide yes)
					(name "PGND")
					(number "21")
				)
				(pin passive line
					(at 24.13 -30.48 180)
					(length 2.54)
					(hide yes)
					(name "PGND")
					(number "22")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 2.54)
					(name "SW")
					(number "23")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "24")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "25")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "26")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "27")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "28")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "29")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "30")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "31")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "32")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "33")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "34")
				)
				(pin passive line
					(at 24.13 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "NC1")
					(number "35")
				)
				(pin output line
					(at 24.13 -10.16 180)
					(length 2.54)
					(name "PGOOD")
					(number "36")
				)
				(pin no_connect line
					(at 21.59 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "NC2")
					(number "37")
				)
				(pin passive line
					(at 24.13 -33.02 180)
					(length 2.54)
					(name "NC1")
					(number "38")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "RSC")
					(number "39")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "SS_TR")
					(number "40")
				)
				(pin passive line
					(at 24.13 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "NC1")
					(number "41")
				)
				(pin input line
					(at 24.13 -5.08 180)
					(length 2.54)
					(name "VSNS+")
					(number "42")
				)
				(pin bidirectional line
					(at 24.13 -15.24 180)
					(length 2.54)
					(name "COMP")
					(number "43")
				)
				(pin output line
					(at 24.13 -20.32 180)
					(length 2.54)
					(name "REFCAP")
					(number "44")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "THERMAL_PAD")
					(number "45")
				)
			)
			(embedded_fonts no)
		)
)
