(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "UCD9081"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.862 -2.032 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "UCD9081"
				(at 38.862 -7.112 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "UCD9081"
				(at 38.862 -9.652 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/gpn/ucd9081"
				(at 38.862 -12.192 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "8-Channel Power Supply Sequencer and Monitor With Error Logging"
				(at 38.862 -22.352 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 38.862 -14.732 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "UCD9081RHBR"
				(at 38.862 -4.572 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 38.862 -17.272 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.862 -19.812 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, POWER, SEQUENCER, I2C"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "UCD9081_1_0"
				(pin no_connect line
					(at 26.67 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "XIN")
					(number "3")
				)
				(pin free line
					(at 0 -31.75 0)
					(length 2.54)
					(name "NC1")
					(number "4")
				)
				(pin input line
					(at 29.21 -2.54 180)
					(length 2.54)
					(name "MON1")
					(number "6")
				)
				(pin input line
					(at 29.21 -7.62 180)
					(length 2.54)
					(name "MON2")
					(number "7")
				)
				(pin input line
					(at 29.21 -12.7 180)
					(length 2.54)
					(name "MON3")
					(number "8")
				)
				(pin input line
					(at 29.21 -27.94 180)
					(length 2.54)
					(name "MON6")
					(number "9")
				)
				(pin output line
					(at 29.21 -15.24 180)
					(length 2.54)
					(name "EN4")
					(number "10")
				)
				(pin output line
					(at 29.21 -10.16 180)
					(length 2.54)
					(name "EN3")
					(number "11")
				)
				(pin output line
					(at 29.21 -20.32 180)
					(length 2.54)
					(name "EN5")
					(number "12")
				)
				(pin output line
					(at 29.21 -25.4 180)
					(length 2.54)
					(name "EN6")
					(number "13")
				)
				(pin output line
					(at 29.21 -30.48 180)
					(length 2.54)
					(name "EN7")
					(number "14")
				)
				(pin input line
					(at 29.21 -33.02 180)
					(length 2.54)
					(name "MON7")
					(number "15")
				)
				(pin input line
					(at 29.21 -38.1 180)
					(length 2.54)
					(name "MON8")
					(number "16")
				)
				(pin free line
					(at 0 -34.29 0)
					(length 2.54)
					(name "NC2")
					(number "17")
				)
				(pin input line
					(at 29.21 -17.78 180)
					(length 2.54)
					(name "MON4")
					(number "18")
				)
				(pin input line
					(at 29.21 -22.86 180)
					(length 2.54)
					(name "MON5")
					(number "19")
				)
				(pin free line
					(at 0 -36.83 0)
					(length 2.54)
					(name "NC3")
					(number "20")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 2.54)
					(name "SDA")
					(number "21")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 2.54)
					(name "SCL")
					(number "22")
				)
				(pin output line
					(at 29.21 0 180)
					(length 2.54)
					(name "EN1")
					(number "23")
				)
				(pin output line
					(at 29.21 -5.08 180)
					(length 2.54)
					(name "EN2")
					(number "24")
				)
				(pin output line
					(at 29.21 -35.56 180)
					(length 2.54)
					(name "GPO1/ADDR1/EN8")
					(number "25")
				)
				(pin output line
					(at 29.21 -41.91 180)
					(length 2.54)
					(name "ADDR2/GPO2")
					(number "26")
				)
				(pin output line
					(at 29.21 -44.45 180)
					(length 2.54)
					(name "ADDR3/GPO3")
					(number "27")
				)
				(pin output line
					(at 29.21 -46.99 180)
					(length 2.54)
					(name "ADDR4/GPO4")
					(number "28")
				)
				(pin passive line
					(at 0 -41.91 0)
					(length 2.54)
					(name "TEST")
					(number "29")
				)
				(pin free line
					(at 0 -39.37 0)
					(length 2.54)
					(name "NC4")
					(number "31")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "ROSC")
					(number "32")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 2.54)
					(name "PAD")
					(number "33")
				)
			)
			(symbol "UCD9081_1_1"
				(pin power_in line
					(at 0 -46.99 0)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "~{RST}")
					(number "5")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "30")
				)
			)
			(embedded_fonts no)
		)
)
