(footprint "BGA-25_5x5_2.075x2.075mm"
	(version 20260206)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Nordic BGA-25_5x5_2.075x2.075mm, 2.075x2.075mm, 25 Ball, 5x5 Layout, 0.4mm Pitch, generated with kicad-footprint-generator ipc_bga_generator.py, https://docs-be.nordicsemi.com/bundle/ps_npm1100/attach/nPM1100_PS_v1.4.pdf?_LANG=enus")
	(tags "BGA 25 0.4")
	(property "Reference" "REF**"
		(at 0 -2.0375 0)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-25_5x5_2.075x2.075mm"
		(at 0 2.0375 0)
		(layer "F.Fab")
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -0.8 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -0.4 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at 0 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at 0.4 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at 0.8 -0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -0.8 -0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -0.4 -0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at 0 -0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at 0.4 -0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at 0.8 -0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -0.8 0)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -0.4 0)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at 0 0)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at 0.4 0)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C5" smd circle
		(at 0.8 0)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -0.8 0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -0.4 0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at 0 0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd circle
		(at 0.4 0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D5" smd circle
		(at 0.8 0.4)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -0.8 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -0.4 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at 0 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd circle
		(at 0.4 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E5" smd circle
		(at 0.8 0.8)
		(size 0.225 0.225)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "nordic_npm1100_caxx.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
