(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "nPM1100-CAXX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 0 0)
				(do_not_autoplace)
			)
			(property "Value" "nPM1100-CAXX"
				(at 0 -2.54 0)
				(do_not_autoplace)
			)
			(property "Footprint" "nordic-lib-kicad-npm:BGA-25_5x5_2.075x2.075mm"
				(at 0 -43.18 0)
			)
			(property "Datasheet" "https://docs-be.nordicsemi.com/bundle/ps_npm1100/attach/nPM1100_PS_v1.4.pdf?_LANG=enus"
				(at 0 -45.72 0)
			)
			(property "Description" "PMIC and Battery Charger, BGA-25"
				(at 0 -40.64 0)
			)
			(property "ki_keywords" "PMIC Charger Regulator"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "BGA?*?*?2.075x2.075mm*"
				(at 0 0 0)
			)
			(symbol "nPM1100-CAXX_0_0"
				(pin bidirectional line
					(at -25.4 12.7 0)
					(length 5.08)
					(name "D+")
					(number "A2")
				)
				(pin bidirectional line
					(at -25.4 10.16 0)
					(length 5.08)
					(name "D-")
					(number "A1")
				)
				(pin passive line
					(at -25.4 2.54 0)
					(length 5.08)
					(name "NTC")
					(number "E1")
				)
				(pin passive line
					(at -25.4 -5.08 0)
					(length 5.08)
					(name "VTERMSET")
					(number "C3")
				)
				(pin passive line
					(at -25.4 -7.62 0)
					(length 5.08)
					(name "ICHG")
					(number "E2")
				)
				(pin passive line
					(at -25.4 -12.7 0)
					(length 5.08)
					(name "ERR")
					(number "E3")
				)
				(pin passive line
					(at -25.4 -15.24 0)
					(length 5.08)
					(name "CHG")
					(number "E4")
				)
				(pin power_in line
					(at -7.62 30.48 270)
					(length 5.08)
					(name "VBAT")
					(number "D1")
				)
				(pin power_in line
					(at 0 30.48 270)
					(length 5.08)
					(name "VBUS")
					(number "B1")
				)
				(pin power_out line
					(at 7.62 30.48 270)
					(length 5.08)
					(name "VSYS")
					(number "C1")
				)
				(pin passive line
					(at 25.4 12.7 180)
					(length 5.08)
					(name "DEC")
					(number "A3")
				)
				(pin passive line
					(at 25.4 7.62 180)
					(length 5.08)
					(name "VOUTBSET1")
					(number "B3")
				)
				(pin power_out line
					(at 25.4 5.08 180)
					(length 5.08)
					(name "VOUTB")
					(number "B5")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 5.08)
					(name "SW")
					(number "A4")
				)
				(pin passive line
					(at 25.4 -5.08 180)
					(length 5.08)
					(name "MODE")
					(number "E5")
				)
				(pin passive line
					(at 25.4 -7.62 180)
					(length 5.08)
					(name "ISET")
					(number "D5")
				)
				(pin input line
					(at 25.4 -12.7 180)
					(length 5.08)
					(name "SHPACT")
					(number "D4")
				)
				(pin input line
					(at 25.4 -15.24 180)
					(length 5.08)
					(name "SHPHLD")
					(number "D3")
				)
			)
			(symbol "nPM1100-CAXX_1_0"
				(pin passive line
					(at -7.62 30.48 270)
					(length 5.08)
					(hide yes)
					(name "VBAT")
					(number "D2")
				)
				(pin passive line
					(at 0 30.48 270)
					(length 5.08)
					(hide yes)
					(name "VBUS")
					(number "B2")
				)
				(pin power_in line
					(at 0 -30.48 90)
					(length 5.08)
					(name "VSS")
					(number "A5")
				)
				(pin passive line
					(at 0 -30.48 90)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "C4")
				)
				(pin passive line
					(at 0 -30.48 90)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "C5")
				)
				(pin passive line
					(at 7.62 30.48 270)
					(length 5.08)
					(hide yes)
					(name "VSYS")
					(number "C2")
				)
				(pin passive line
					(at 25.4 10.16 180)
					(length 5.08)
					(name "VOUTBSET0")
					(number "B4")
				)
			)
			(symbol "nPM1100-CAXX_1_1")
			(embedded_fonts no)
		)
)
