(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "nPM1300-CAXX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 0 0)
				(do_not_autoplace)
			)
			(property "Value" "nPM1300-CAXX"
				(at 0 -2.54 0)
				(do_not_autoplace)
			)
			(property "Footprint" "nordic-lib-kicad-npm:BGA-35_7x5_3.077x2.3775mm"
				(at 0 -58.42 0)
			)
			(property "Datasheet" "https://docs.nordicsemi.com/bundle/ps_npm1300"
				(at 0 -55.88 0)
			)
			(property "Description" "PMIC, LED Driver, Battery Charger, BGA-35"
				(at 0 -53.34 0)
			)
			(property "ki_keywords" "PMIC Regulator LED Driver Battery Charger"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "BGA*35*7x5*3.077x2.3775mm*"
				(at 0 0 0)
			)
			(symbol "nPM1300-CAXX_0_0"
				(pin bidirectional line
					(at -35.56 0 0)
					(length 5.08)
					(name "GPIO1")
					(number "E6")
				)
				(pin bidirectional line
					(at -35.56 -2.54 0)
					(length 5.08)
					(name "GPIO2")
					(number "C5")
				)
				(pin bidirectional line
					(at -35.56 -5.08 0)
					(length 5.08)
					(name "GPIO3")
					(number "C4")
				)
			)
			(symbol "nPM1300-CAXX_1_0"
				(pin power_in line
					(at -35.56 33.02 0)
					(length 5.08)
					(name "VBUS")
					(number "B1")
				)
				(pin passive line
					(at -35.56 33.02 0)
					(length 5.08)
					(hide yes)
					(name "VBUS")
					(number "B2")
				)
				(pin bidirectional line
					(at -35.56 20.32 0)
					(length 5.08)
					(name "CC1")
					(number "D5")
				)
				(pin bidirectional line
					(at -35.56 17.78 0)
					(length 5.08)
					(name "CC2")
					(number "B3")
				)
				(pin open_collector line
					(at -35.56 12.7 0)
					(length 5.08)
					(name "LED0")
					(number "A1")
				)
				(pin open_collector line
					(at -35.56 10.16 0)
					(length 5.08)
					(name "LED1")
					(number "A2")
				)
				(pin open_collector line
					(at -35.56 7.62 0)
					(length 5.08)
					(name "LED2")
					(number "A3")
				)
				(pin bidirectional line
					(at -35.56 2.54 0)
					(length 5.08)
					(name "GPIO0")
					(number "D6")
				)
				(pin bidirectional line
					(at -35.56 -12.7 0)
					(length 5.08)
					(name "SDA")
					(number "E5")
				)
				(pin bidirectional line
					(at -35.56 -15.24 0)
					(length 5.08)
					(name "SCL")
					(number "E3")
				)
				(pin passive line
					(at -35.56 -20.32 0)
					(length 5.08)
					(name "VSET1")
					(number "E2")
				)
				(pin passive line
					(at -35.56 -22.86 0)
					(length 5.08)
					(name "VSET2")
					(number "E1")
				)
				(pin passive line
					(at -35.56 -27.94 0)
					(length 5.08)
					(name "SHPHLD")
					(number "D4")
				)
				(pin power_in line
					(at -2.54 40.64 270)
					(length 5.08)
					(name "VDDIO")
					(number "E4")
				)
				(pin power_in line
					(at 0 40.64 270)
					(length 5.08)
					(name "PVDD")
					(number "C7")
				)
				(pin power_in line
					(at 0 -40.64 90)
					(length 5.08)
					(name "VSS")
					(number "A6")
				)
				(pin power_out line
					(at 2.54 40.64 270)
					(length 5.08)
					(name "VSYS")
					(number "C1")
				)
				(pin passive line
					(at 2.54 40.64 270)
					(length 5.08)
					(hide yes)
					(name "VSYS")
					(number "C2")
				)
				(pin power_out line
					(at 35.56 33.02 180)
					(length 5.08)
					(name "VBUSOUT")
					(number "C3")
				)
				(pin power_out line
					(at 35.56 17.78 180)
					(length 5.08)
					(name "VOUT1")
					(number "B6")
				)
				(pin passive line
					(at 35.56 12.7 180)
					(length 5.08)
					(name "SW1")
					(number "B7")
				)
				(pin power_in line
					(at 35.56 10.16 180)
					(length 5.08)
					(name "PVSS1")
					(number "A7")
				)
				(pin power_out line
					(at 35.56 5.08 180)
					(length 5.08)
					(name "VOUT2")
					(number "C6")
				)
				(pin passive line
					(at 35.56 0 180)
					(length 5.08)
					(name "SW2")
					(number "D7")
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "PVSS2")
					(number "E7")
				)
				(pin input line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "LSIN1/VINLDO1")
					(number "B4")
				)
				(pin output line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "LSOUT1/VOUTLDO1")
					(number "A4")
				)
				(pin input line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "LSIN2/VINLDO2")
					(number "B5")
				)
				(pin output line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "LSOUT2/VOUTLDO2")
					(number "A5")
				)
				(pin power_in line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "VBAT")
					(number "D1")
				)
				(pin passive line
					(at 35.56 -30.48 180)
					(length 5.08)
					(hide yes)
					(name "VBAT")
					(number "D2")
				)
				(pin passive line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "NTC")
					(number "D3")
				)
			)
			(symbol "nPM1300-CAXX_1_1")
			(embedded_fonts no)
		)
)
