(footprint "BGA-16_4x4_1.9175x1.8975mm"
	(version 20260206)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Nordic BGA-16_4x4_1.9175x1.8975mm, 1.9175x1.8975mm, 16 Ball, 4x4 Layout, 0.44mm Pitch, generated with kicad-footprint-generator ipc_bga_generator.py, https://www.nordicsemi.com/products/nPM2100")
	(tags "BGA 16 0.44")
	(property "Reference" "REF**"
		(at 0 -1.94875 0)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-16_4x4_1.9175x1.8975mm"
		(at 0 1.94875 0)
		(layer "F.Fab")
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -0.66 -0.66)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -0.22 -0.66)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at 0.22 -0.66)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at 0.66 -0.66)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -0.66 -0.22)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -0.22 -0.22)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at 0.22 -0.22)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at 0.66 -0.22)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -0.66 0.22)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -0.22 0.22)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at 0.22 0.22)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at 0.66 0.22)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -0.66 0.66)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -0.22 0.66)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at 0.22 0.66)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd circle
		(at 0.66 0.66)
		(size 0.22 0.22)
		(property pad_prop_bga)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "nordic_npm2100_caxx.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
