(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Relay_DPDT_EC2-12NU"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "K"
				(at 25.4 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Relay_DPDT_EC2-12NU"
				(at 25.4 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Relay_DPDT_EC2-12NU"
				(at 25.4 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/447/KEM_R7002_EC2_EE2-3316920.pdf"
				(at 25.4 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Relay, DPDT, 12VDC, 2A"
				(at 25.4 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "KEMET"
				(at 25.4 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "EC2-12NU"
				(at 25.4 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 25.4 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 25.4 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "RELAY, DPDT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Relay_DPDT_EC2-12NU_1_1"
				(pin passive line
					(at 12.7 0 180)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 12.7 -6.35 180)
					(length 2.54)
					(name "NC1")
					(number "3")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "COM1")
					(number "4")
				)
				(pin passive line
					(at 12.7 -3.81 180)
					(length 2.54)
					(name "NO1")
					(number "5")
				)
				(pin passive line
					(at 12.7 -10.16 180)
					(length 2.54)
					(name "NO2")
					(number "8")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 2.54)
					(name "COM2")
					(number "9")
				)
				(pin passive line
					(at 12.7 -12.7 180)
					(length 2.54)
					(name "NC2")
					(number "10")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "12")
				)
			)
			(embedded_fonts no)
		)
)
