(footprint "REL_ENERDIS_OKTMS4R"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "16 Leads, Row Spacing 10mm; Body 45mm x 53mm, 4 x DPDT Relay, ENERDIS F-OK Series")
	(property "Reference" "REF**"
		(at 0 -23.30001 0)
		(layer "F.SilkS")
	)
	(property "Value" "REL_ENERDIS_OKTMS4R"
		(at 0 23.30001 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "5A"
		(at 16.17501 -17.19733 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "8B"
		(at -13.75001 -17.16626 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "5B"
		(at -3.75001 -17.19733 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6A"
		(at 6.21988 4.46741 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3B"
		(at -3.75001 4.40269 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3A"
		(at 16.17501 4.40269 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4A"
		(at 16.10001 -7.16626 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1B"
		(at -3.32501 16.75876 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "7B"
		(at -13.75001 -7.16626 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1A"
		(at 16.17501 14.40269 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2B"
		(at -13.82501 14.40269 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6B"
		(at -13.70513 4.46741 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "8A"
		(at 6.175 -17.16626 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4B"
		(at -3.825 -7.16626 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2A"
		(at 6.175 14.40269 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "7A"
		(at 6.175 -7.16626 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "Use with Socket ENERDIS 65F-P01400153A"
		(at -16.471055 11.853945 45)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "8B"
		(at -13.75001 -17.16626 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "4B"
		(at -3.825 -7.16626 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5A"
		(at 16.17501 -17.19733 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "6A"
		(at 6.21988 4.46741 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "4A"
		(at 16.10001 -7.16626 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "7A"
		(at 6.175 -7.16626 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "3A"
		(at 16.17501 4.40269 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1A"
		(at 16.17501 14.40269 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "7B"
		(at -13.75001 -7.16626 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "2B"
		(at -13.82501 14.40269 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5B"
		(at -3.75001 -17.19733 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "3B"
		(at -3.75001 4.40269 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "6B"
		(at -13.70513 4.46741 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "8A"
		(at 6.175 -17.16626 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1B"
		(at -3.32501 16.75876 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "2A"
		(at 6.175 14.40269 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 3.9 3.9)
		(drill 3.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "1A" thru_hole circle
		(at 15.00001 15.80001)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "1B" thru_hole circle
		(at -5 15.80001)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 17.50001 0)
		(size 3.9 3.9)
		(drill 3.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2A" thru_hole circle
		(at 5 15.80001)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2B" thru_hole circle
		(at -15.00001 15.80001)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3A" thru_hole circle
		(at 15.00001 5.8)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3B" thru_hole circle
		(at -5 5.8)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4A" thru_hole circle
		(at 15.00001 -5.8)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4B" thru_hole circle
		(at -5 -5.8)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5A" thru_hole circle
		(at 15.00001 -15.80001)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5B" thru_hole circle
		(at -5 -15.80001)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6A" thru_hole circle
		(at 5 5.8)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6B" thru_hole circle
		(at -15.00001 5.8)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7A" thru_hole circle
		(at 5 -5.8)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7B" thru_hole circle
		(at -15.00001 -5.8)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8A" thru_hole circle
		(at 5 -15.80001)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8B" thru_hole circle
		(at -15.00001 -15.80001)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
