(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "REL_ENERDIS_OKTMS4R"
  		(pin_names
  			(offset 1.27)
  			(hide yes)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "RL"
  			(at 5.08 5.08 0)
  		)
  		(property "Value" "*"
  			(at 2.286 -3.048 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "10A, 4 Changeover Contacts, Programmable Off Time-Delay Relay, ENERDIS OK tms Serie"
  			(at 0 0 0)
  		)
  		(symbol "REL_ENERDIS_OKTMS4R_1_0"
  			(text "+"
  				(at 2.032 1.016 0)
  			)
  			(pin passive line
  				(at 0 1.27 0)
  				(length 2.54)
  				(name "1B")
  				(number "1B")
  			)
  			(pin passive line
  				(at 0 -1.27 0)
  				(length 2.54)
  				(name "2B")
  				(number "2B")
  			)
  			(pin passive line
  				(at 10.16 0 180)
  				(length 1.27)
  				(name "1A")
  				(number "1A")
  			)
  		)
  		(symbol "REL_ENERDIS_OKTMS4R_2_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "3B")
  				(number "3B")
  			)
  			(pin bidirectional line
  				(at 15.24 2.54 180)
  				(length 4.445)
  				(name "4B")
  				(number "4B")
  			)
  			(pin bidirectional line
  				(at 15.24 -2.54 180)
  				(length 4.445)
  				(name "5B")
  				(number "5B")
  			)
  		)
  		(symbol "REL_ENERDIS_OKTMS4R_3_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "6B")
  				(number "6B")
  			)
  			(pin bidirectional line
  				(at 15.24 2.54 180)
  				(length 4.445)
  				(name "7B")
  				(number "7B")
  			)
  			(pin bidirectional line
  				(at 15.24 -2.54 180)
  				(length 4.445)
  				(name "8B")
  				(number "8B")
  			)
  		)
  		(symbol "REL_ENERDIS_OKTMS4R_4_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "3A")
  				(number "3A")
  			)
  			(pin bidirectional line
  				(at 15.24 2.54 180)
  				(length 4.445)
  				(name "4A")
  				(number "4A")
  			)
  			(pin bidirectional line
  				(at 15.24 -2.54 180)
  				(length 4.445)
  				(name "5A")
  				(number "5A")
  			)
  		)
  		(symbol "REL_ENERDIS_OKTMS4R_5_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "6A")
  				(number "6A")
  			)
  			(pin bidirectional line
  				(at 15.24 2.54 180)
  				(length 4.445)
  				(name "7A")
  				(number "7A")
  			)
  			(pin bidirectional line
  				(at 15.24 -2.54 180)
  				(length 4.445)
  				(name "8A")
  				(number "8A")
  			)
  		)
  		(embedded_fonts no)
  	)
)
