(footprint "REL_MEDER_CRF"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "10 Pin SPST Relay, MEDER CRF Series, Body 8.6mm x 4.4mm")
	(property "Reference" "REF**"
		(at 0 -3.175 0)
		(layer "F.SilkS")
	)
	(property "Value" "REL_MEDER_CRF"
		(at 0 3.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -4.55 1.71)
		(size 0.5 0.98)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd custom
		(at -4.3 1.22)
		(size 0.000001 0.000001)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0 0.98) (xy 0.83227 0.74142) (xy 0.92497 0.71484) (xy 1.07545 0.59422) (xy 1.16767 0.42484) (xy 1.18732 0.23299) (xy 1.13136 0.04843) (xy 1.00846 -0.10019) (xy 0.83769 -0.18982) (xy 0.64556 -0.20655) (xy 0.55372 -0.17716) (xy 0.55372 -0.17717)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at -1.67 1.3)
		(size 0.000001 0.000001)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0 -0.09449) (xy 0.07232 -0.26907) (xy 0.20594 -0.40269) (xy 0.38052 -0.475) (xy 0.56949 -0.475) (xy 0.74407 -0.40269) (xy 0.87769 -0.26907) (xy 0.95 -0.09449) (xy 0.95 0)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd rect
		(at -1.2 1.9)
		(size 0.98 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd custom
		(at 0.72 1.3)
		(size 0.000001 0.000001)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0 -0.09449) (xy 0.07231 -0.26907) (xy 0.20593 -0.40269) (xy 0.38051 -0.475) (xy 0.56948 -0.475) (xy 0.74406 -0.40269) (xy 0.87768 -0.26907) (xy 0.95 -0.09449) (xy 0.95 0)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "3" smd rect
		(at 1.2 1.9)
		(size 0.98 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd custom
		(at 4.3 1.22)
		(size 0.000001 0.000001)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0 0.98) (xy -0.83227 0.74142) (xy -0.92497 0.71484) (xy -1.07545 0.59422) (xy -1.16767 0.42484) (xy -1.18733 0.23299) (xy -1.13136 0.04843) (xy -1.00846 -0.10019) (xy -0.8377 -0.18983) (xy -0.64556 -0.20655) (xy -0.55372 -0.17717)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "4" smd rect
		(at 4.55 1.71)
		(size 0.5 0.98)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd custom
		(at 4.3 -0.72)
		(size 0.000001 0.000001)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0 1.44) (xy -0.84236 1.1784) (xy -0.91573 1.15562) (xy -1.04092 1.06652) (xy -1.13204 0.94281) (xy -1.18 0.79683) (xy -1.18 0.64317) (xy -1.13204 0.4972) (xy -1.04092 0.37348) (xy -0.91573 0.28438) (xy -0.84236 0.2616)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "5" smd rect
		(at 4.55 0)
		(size 0.5 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd custom
		(at 4.3 -1.22)
		(size 0.000001 0.000001)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0 -0.98) (xy -0.83227 -0.74141) (xy -0.92497 -0.71484) (xy -1.07545 -0.59422) (xy -1.16768 -0.42484) (xy -1.18733 -0.23299) (xy -1.13137 -0.04843) (xy -1.00847 0.1002) (xy -0.8377 0.18983) (xy -0.64557 0.20655) (xy -0.55373 0.17717) (xy -0.55372 0.17717)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "6" smd rect
		(at 4.55 -1.71)
		(size 0.5 0.98)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd circle
		(at 1.195 -1.5)
		(size 0.95 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
	)
	(pad "8" smd circle
		(at -1.195 -1.5)
		(size 0.95 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
	)
	(pad "9" smd rect
		(at -4.55 -1.71)
		(size 0.5 0.98)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd custom
		(at -4.3 -1.22)
		(size 0.000001 0.000001)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0 -0.98) (xy 0.83227 -0.74141) (xy 0.92497 -0.71484) (xy 1.07545 -0.59422) (xy 1.16767 -0.42484) (xy 1.18733 -0.23299) (xy 1.13136 -0.04843) (xy 1.00846 0.1002) (xy 0.8377 0.18983) (xy 0.64557 0.20655) (xy 0.55372 0.17717)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "10" smd rect
		(at -4.55 0)
		(size 0.5 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd custom
		(at -4.3 0.72)
		(size 0.000001 0.000001)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0 -1.44) (xy 0.84236 -1.1784) (xy 0.91573 -1.15562) (xy 1.04092 -1.06652) (xy 1.13204 -0.9428) (xy 1.18 -0.79683) (xy 1.18 -0.64317) (xy 1.13204 -0.49719) (xy 1.04092 -0.37348) (xy 0.91573 -0.28438) (xy 0.84236 -0.2616)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
)
