(footprint "REL_MEDER_CRF-S"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "10 Pin SPST BGA Relay, MEDER CRF Series, Body 8.6mm x 4.4mm")
	(property "Reference" "REF**"
		(at 0 -3.175 0)
		(layer "F.SilkS")
	)
	(property "Value" "REL_MEDER_CRF-S"
		(at 0 3.71569 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd circle
		(at -3.6 1.5)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
	)
	(pad "2" smd circle
		(at -1.2 1.5)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
	)
	(pad "3" smd circle
		(at 1.2 1.5)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
	)
	(pad "4" smd circle
		(at 3.6 1.5)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
	)
	(pad "5" smd circle
		(at 3.6 0)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
	)
	(pad "6" smd circle
		(at 3.6 -1.5)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
	)
	(pad "7" smd circle
		(at 1.2 -1.5)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
	)
	(pad "8" smd circle
		(at -1.2 -1.5)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
	)
	(pad "9" smd circle
		(at -3.6 -1.5)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
	)
	(pad "10" smd circle
		(at -3.6 0)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
