(footprint "REL_PANASONIC_AGQ200A"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "8 Leads Single Side Stable Relay,PANASONIC GQ Series, Body 10.6mm x 7.2mm")
	(property "Reference" "REF**"
		(at 0 -5.675 0)
		(layer "F.SilkS")
	)
	(property "Value" "REL_PANASONIC_AGQ200A"
		(at 0 5.675 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -3.8 3.37)
		(size 0.8 2.66)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.6 3.37)
		(size 0.8 2.66)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 1.6 3.37)
		(size 0.8 2.66)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 3.8 3.37)
		(size 0.8 2.66)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 3.8 -3.37)
		(size 0.8 2.66)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.6 -3.37)
		(size 0.8 2.66)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -0.6 -3.37)
		(size 0.8 2.66)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -3.8 -3.37)
		(size 0.8 2.66)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
