(footprint "REL_PANASONIC_S2"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "12 Leads Single Side Stable Relay, PANASONIC S Series, Body 29mm x 12mm x 10.9mm H")
	(property "Reference" "REF**"
		(at -0.25 -6.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "REL_PANASONIC_S2"
		(at -0.25 6.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "9"
		(at 2.17317 -1.21155 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "1"
		(at -12.95 2.4325 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "11"
		(at -8.12 -1.1875 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "3"
		(at -2.91071 2.41179 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "5"
		(at 7.24541 2.41179 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "4"
		(at 2.14 2.4325 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "12"
		(at -13.33003 -1.1624 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "2"
		(at -7.98733 2.4576 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "7"
		(at 12.36682 -1.1875 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "10"
		(at -3.14039 -1.1875 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "8"
		(at 7.26721 -1.1875 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "6"
		(at 12.35512 2.45494 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(pad "1" thru_hole rect
		(at -12.7 3.81)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -7.62 3.81)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at -2.54 3.81)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at 2.54 3.81)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at 7.62 3.81)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at 12.7 3.81)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at 12.7 -3.81)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at 7.62 -3.81)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "9" thru_hole circle
		(at 2.54 -3.81)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "10" thru_hole circle
		(at -2.54 -3.81)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "11" thru_hole circle
		(at -7.62 -3.81)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "12" thru_hole circle
		(at -12.7 -3.81)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
