(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "REL_PANASONIC_S2"
  		(pin_names
  			(offset 1.27)
  			(hide yes)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "RL"
  			(at 5.08 3.81 0)
  		)
  		(property "Value" "*"
  			(at 2.286 -3.048 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "12 Leads Single Side Stable Relay, PANASONIC S Series, Body 29mm x 12mm x 10.5mm H"
  			(at 0 0 0)
  		)
  		(symbol "REL_PANASONIC_S2_1_0"
  			(text "+"
  				(at 2.286 0.254 0)
  			)
  			(pin passive line
  				(at 0 0 0)
  				(length 3.81)
  				(name "COIL+")
  				(number "1")
  			)
  			(pin passive line
  				(at 10.16 0 180)
  				(length 3.81)
  				(name "COIL-")
  				(number "12")
  			)
  		)
  		(symbol "REL_PANASONIC_S2_2_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "3")
  			)
  			(pin bidirectional line
  				(at 15.24 0 180)
  				(length 4.445)
  				(name "NO")
  				(number "2")
  			)
  		)
  		(symbol "REL_PANASONIC_S2_3_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "4")
  			)
  			(pin bidirectional line
  				(at 15.24 0 180)
  				(length 4.445)
  				(name "NO")
  				(number "5")
  			)
  		)
  		(symbol "REL_PANASONIC_S2_4_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "9")
  			)
  			(pin bidirectional line
  				(at 15.24 0 180)
  				(length 4.445)
  				(name "NO")
  				(number "8")
  			)
  		)
  		(symbol "REL_PANASONIC_S2_5_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "10")
  			)
  			(pin bidirectional line
  				(at 15.24 0 180)
  				(length 4.445)
  				(name "NO")
  				(number "11")
  			)
  		)
  		(embedded_fonts no)
  	)
)
