(footprint "REL_PANASONIC_SF4D"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "18 Leads, Flat Type Safety Relay, Body 53.3mm x 33mm, SF Series")
	(property "Reference" "REF**"
		(at 0.000005 -17.29997 0)
		(layer "F.SilkS")
	)
	(property "Value" "REL_PANASONIC_SF4D"
		(at 0.000005 17.29998 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "14"
		(at -7.785 14.90377 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "12"
		(at 17.64502 -5.41617 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "11"
		(at 10.64003 -5.41617 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "9"
		(at -14.56029 -5.41617 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "8"
		(at 18.56507 7.28379 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "18"
		(at -7.71 -13.03615 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "19"
		(at 10.43634 -13.03615 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "2"
		(at -24.64106 -2.87618 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at -6.82732 7.28379 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1+"
		(at -25.49006 4.7438 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "10"
		(at -7.71059 -5.41617 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "20"
		(at 17.55852 -13.03615 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "17"
		(at -14.91004 -13.03615 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "7"
		(at 10.86503 7.28379 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "15"
		(at 10.45897 14.90377 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "16"
		(at 17.65286 14.90377 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "13"
		(at -14.94111 14.90377 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5"
		(at -14.56611 7.28379 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -21.59006 3.81005)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -21.59006 -3.80993)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -16.51004 6.35004)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at -3.81 6.35004)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at 8.89003 6.35004)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at 21.59007 6.35004)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "9" thru_hole circle
		(at -16.51004 -6.34992)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "10" thru_hole circle
		(at -3.81 -6.34992)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "11" thru_hole circle
		(at 8.89003 -6.34992)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "12" thru_hole circle
		(at 21.59007 -6.34992)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "13" thru_hole circle
		(at -16.51004 13.97002)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "14" thru_hole circle
		(at -3.81 13.97002)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "15" thru_hole circle
		(at 8.89003 13.97002)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "16" thru_hole circle
		(at 21.59007 13.97002)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "17" thru_hole circle
		(at -16.51004 -13.9699)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "18" thru_hole circle
		(at -3.81 -13.9699)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "19" thru_hole circle
		(at 8.89003 -13.9699)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "20" thru_hole circle
		(at 21.59007 -13.9699)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
