(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "REL_PANASONIC_SF4D"
  		(pin_names
  			(offset 1.27)
  			(hide yes)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "RL"
  			(at 5.08 3.81 0)
  		)
  		(property "Value" "*"
  			(at 2.286 -3.048 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "6A 250VAC, 4 Form A (SPST-NO) + 4 Form B (SPST-NC), Flat Type Safety Relay, SF Series"
  			(at 0 0 0)
  		)
  		(symbol "REL_PANASONIC_SF4D_1_0"
  			(text "+"
  				(at 2.286 0.254 0)
  			)
  			(pin passive line
  				(at 0 0 0)
  				(length 3.81)
  				(name "COIL+")
  				(number "1")
  			)
  			(pin passive line
  				(at 10.16 0 180)
  				(length 3.81)
  				(name "COIL-")
  				(number "2")
  			)
  		)
  		(symbol "REL_PANASONIC_SF4D_2_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "6")
  			)
  			(pin bidirectional line
  				(at 15.24 0 180)
  				(length 4.445)
  				(name "NC")
  				(number "5")
  			)
  		)
  		(symbol "REL_PANASONIC_SF4D_3_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "7")
  			)
  			(pin bidirectional line
  				(at 15.24 0 180)
  				(length 4.445)
  				(name "NO")
  				(number "8")
  			)
  		)
  		(symbol "REL_PANASONIC_SF4D_4_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "10")
  			)
  			(pin bidirectional line
  				(at 15.24 0 180)
  				(length 4.445)
  				(name "NO")
  				(number "9")
  			)
  		)
  		(symbol "REL_PANASONIC_SF4D_5_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "11")
  			)
  			(pin bidirectional line
  				(at 15.24 0 180)
  				(length 4.445)
  				(name "NC")
  				(number "12")
  			)
  		)
  		(symbol "REL_PANASONIC_SF4D_6_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "14")
  			)
  			(pin bidirectional line
  				(at 15.24 0 180)
  				(length 4.445)
  				(name "NO")
  				(number "13")
  			)
  		)
  		(symbol "REL_PANASONIC_SF4D_7_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "15")
  			)
  			(pin bidirectional line
  				(at 15.24 0 180)
  				(length 4.445)
  				(name "NC")
  				(number "16")
  			)
  		)
  		(symbol "REL_PANASONIC_SF4D_8_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "18")
  			)
  			(pin bidirectional line
  				(at 15.24 0 180)
  				(length 4.445)
  				(name "NO")
  				(number "17")
  			)
  		)
  		(symbol "REL_PANASONIC_SF4D_9_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "19")
  			)
  			(pin bidirectional line
  				(at 15.24 0 180)
  				(length 4.445)
  				(name "NC")
  				(number "20")
  			)
  		)
  		(embedded_fonts no)
  	)
)
