(footprint "REL_PANASONIC_TQ2SA"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "10 Leads Single Side Stable Relay, SMD, Very High Sensitivity (140mW) PANASONIC TQ Series, Body 14mm x 9mm x 5.6mm H")
	(property "Reference" "REF**"
		(at 0 -6.94999 0)
		(layer "F.SilkS")
	)
	(property "Value" "REL_PANASONIC_TQ2SA"
		(at 0 6.95 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -5.08 4.78)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.54 4.78)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0 4.78)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 2.54 4.78)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 5.08 4.78)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 5.08 -4.77999 180)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 2.54 -4.77999 180)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0 -4.77999 180)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -2.54 -4.77999 180)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -5.08 -4.77999 180)
		(size 1 2.94)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
