(footprint "REL_TYCO_IMXXXGX"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "8 Gull Wings Leads SMT Relay, IM Series, Body 10mm x 6mm")
	(property "Reference" "REF**"
		(at 0 -4.97492 0)
		(layer "F.SilkS")
	)
	(property "Value" "REL_TYCO_IMXXXGX"
		(at 0 4.97508 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -3.79996 3)
		(size 0.7 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.59996 3)
		(size 0.7 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 1.60005 3)
		(size 0.7 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 3.80005 3)
		(size 0.7 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 3.80005 -3)
		(size 0.7 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.60005 -3)
		(size 0.7 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -0.59996 -3)
		(size 0.7 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -3.79996 -3)
		(size 0.7 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
