(footprint "REL_TYCO_PE01"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "1 form C (CO) General Purpose Low Power PCB Relay, PE Series, Body 20mm x 10mm")
	(property "Reference" "REF**"
		(at -0.25 -5.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "REL_TYCO_PE01"
		(at -0.25 5.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "11" thru_hole circle
		(at 1.27 3.81 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "12" thru_hole circle
		(at 8.89 -3.81 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "14" thru_hole circle
		(at 8.89 3.81 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "A1" thru_hole circle
		(at -8.89 3.81 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "A2" thru_hole circle
		(at -8.89 -3.81 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
