(footprint "REL_TYCO_PT5X1"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "4 Poles General Purpose Relay,Body W 22.5x L 28 x H 29mm,PT Series")
	(property "Reference" "REF**"
		(at 0 -14.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "REL_TYCO_PT5X1"
		(at 0 14.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "11" thru_hole circle
		(at 6.6 0.8)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(padstack
			(mode front_inner_back)
			(layer "Inner"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
			(layer "B.Cu"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
		)
	)
	(pad "12" thru_hole circle
		(at 6.6 -9.55)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(padstack
			(mode front_inner_back)
			(layer "Inner"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
			(layer "B.Cu"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
		)
	)
	(pad "14" thru_hole circle
		(at 6.6 -5.55)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(padstack
			(mode front_inner_back)
			(layer "Inner"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
			(layer "B.Cu"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
		)
	)
	(pad "21" thru_hole circle
		(at 2.2 0.8)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(padstack
			(mode front_inner_back)
			(layer "Inner"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
			(layer "B.Cu"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
		)
	)
	(pad "22" thru_hole circle
		(at 2.2 -9.55)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(padstack
			(mode front_inner_back)
			(layer "Inner"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
			(layer "B.Cu"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
		)
	)
	(pad "24" thru_hole circle
		(at 2.2 -5.55)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(padstack
			(mode front_inner_back)
			(layer "Inner"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
			(layer "B.Cu"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
		)
	)
	(pad "31" thru_hole circle
		(at -2.2 0.8)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(padstack
			(mode front_inner_back)
			(layer "Inner"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
			(layer "B.Cu"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
		)
	)
	(pad "32" thru_hole circle
		(at -2.2 -9.55)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(padstack
			(mode front_inner_back)
			(layer "Inner"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
			(layer "B.Cu"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
		)
	)
	(pad "34" thru_hole circle
		(at -2.2 -5.55)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(padstack
			(mode front_inner_back)
			(layer "Inner"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
			(layer "B.Cu"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
		)
	)
	(pad "41" thru_hole circle
		(at -6.6 0.8)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(padstack
			(mode front_inner_back)
			(layer "Inner"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
			(layer "B.Cu"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
		)
	)
	(pad "42" thru_hole circle
		(at -6.6 -9.55)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(padstack
			(mode front_inner_back)
			(layer "Inner"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
			(layer "B.Cu"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
		)
	)
	(pad "44" thru_hole circle
		(at -6.6 -5.55)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(padstack
			(mode front_inner_back)
			(layer "Inner"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
			(layer "B.Cu"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
		)
	)
	(pad "A1" thru_hole circle
		(at 6.6 7.15)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(padstack
			(mode front_inner_back)
			(layer "Inner"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
			(layer "B.Cu"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
		)
	)
	(pad "A2" thru_hole circle
		(at -6.6 7.15)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(padstack
			(mode front_inner_back)
			(layer "Inner"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
			(layer "B.Cu"
				(shape circle)
				(size 2 2)
				(thermal_bridge_angle 90)
				(zone_connect -1)
			)
		)
	)
	(embedded_fonts no)
)
