(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "REL_TYCO_PT5710xx"
  		(pin_names
  			(offset 1.27)
  			(hide yes)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "RL"
  			(at 5.08 3.81 0)
  		)
  		(property "Value" "*"
  			(at 2.286 -3.048 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "6A/240VAC, 4 form C (CO) General Purpose Industrial PCB Relay, PT Series"
  			(at 0 0 0)
  		)
  		(symbol "REL_TYCO_PT5710xx_1_0"
  			(pin passive line
  				(at 0 0 0)
  				(length 3.81)
  				(name "COIL")
  				(number "A1")
  			)
  			(pin passive line
  				(at 10.16 0 180)
  				(length 3.81)
  				(name "COIL")
  				(number "A2")
  			)
  		)
  		(symbol "REL_TYCO_PT5710xx_2_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "11")
  			)
  			(pin bidirectional line
  				(at 15.24 2.54 180)
  				(length 4.445)
  				(name "NC")
  				(number "12")
  			)
  			(pin bidirectional line
  				(at 15.24 -2.54 180)
  				(length 4.445)
  				(name "NO")
  				(number "14")
  			)
  		)
  		(symbol "REL_TYCO_PT5710xx_3_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "21")
  			)
  			(pin bidirectional line
  				(at 15.24 2.54 180)
  				(length 4.445)
  				(name "NC")
  				(number "22")
  			)
  			(pin bidirectional line
  				(at 15.24 -2.54 180)
  				(length 4.445)
  				(name "NO")
  				(number "24")
  			)
  		)
  		(symbol "REL_TYCO_PT5710xx_4_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "31")
  			)
  			(pin bidirectional line
  				(at 15.24 2.54 180)
  				(length 4.445)
  				(name "NC")
  				(number "32")
  			)
  			(pin bidirectional line
  				(at 15.24 -2.54 180)
  				(length 4.445)
  				(name "NO")
  				(number "34")
  			)
  		)
  		(symbol "REL_TYCO_PT5710xx_5_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "41")
  			)
  			(pin bidirectional line
  				(at 15.24 2.54 180)
  				(length 4.445)
  				(name "NC")
  				(number "42")
  			)
  			(pin bidirectional line
  				(at 15.24 -2.54 180)
  				(length 4.445)
  				(name "NO")
  				(number "44")
  			)
  		)
  		(embedded_fonts no)
  	)
)
