(footprint "REL_TYCO_SCHRACK_RT44XXXX"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "6 Leads, Row Spacing 7.5 mm; Body 29mm x 12.7mm, TYCO RT2 Series")
	(property "Reference" "REF**"
		(at 0 -7.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "REL_TYCO_SCHRACK_RT44XXXX"
		(at 0 7.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "11" thru_hole circle
		(at 8.15 3.81 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "14" thru_hole circle
		(at 13.23 3.81 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "21" thru_hole circle
		(at 8.15 -3.81 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "24" thru_hole circle
		(at 13.23 -3.81 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "A1" thru_hole circle
		(at -12.17 3.81 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "A2" thru_hole circle
		(at -12.17 -3.81 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
