(footprint "REL_TYCO_SCHRACK_RYII_CO"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "5 Leads, Row Spacing 7.62 mm; Body 28.5mm x 10.1mm, TYCO RYII Series, CO Contact")
	(property "Reference" "REF**"
		(at 0 -5.85 0)
		(layer "F.SilkS")
	)
	(property "Value" "REL_TYCO_SCHRACK_RYII_CO"
		(at 0 5.85 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "11" thru_hole circle
		(at 9.75001 3.79 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "12" thru_hole circle
		(at 6.55001 -3.79 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "14" thru_hole circle
		(at 12.95001 -3.79 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "A1" thru_hole circle
		(at -12.35001 3.79 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "A2" thru_hole circle
		(at -12.35001 -3.79 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
