(footprint "REL_TYCO_SCHRACK_SR6B"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "14 Leads, Row Spacing 10mm; Body 55mm x 16.5mm, TYCO SR6 Series")
	(property "Reference" "REF**"
		(at 0 -9.05001 0)
		(layer "F.SilkS")
	)
	(property "Value" "REL_TYCO_SCHRACK_SR6B"
		(at 0 9.05001 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "11" thru_hole circle
		(at -2.55 -5 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "12" thru_hole circle
		(at 2.45 -5 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "21" thru_hole circle
		(at -2.55 5 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "22" thru_hole circle
		(at 2.45 5 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "33" thru_hole circle
		(at 13.95001 -5 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "34" thru_hole circle
		(at 8.95001 -5 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "43" thru_hole circle
		(at 13.95001 5 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "44" thru_hole circle
		(at 8.95001 5 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "53" thru_hole circle
		(at 25.45001 -5 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "54" thru_hole circle
		(at 20.45001 -5 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "63" thru_hole circle
		(at 25.45001 5 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "64" thru_hole circle
		(at 20.45001 5 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "A1" thru_hole circle
		(at -25.05001 -6.25 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "A2" thru_hole circle
		(at -25.05001 6.25 90)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
