(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "REL_TYCO_SCHRACK_SR6C"
  		(pin_names
  			(offset 1.27)
  			(hide yes)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "RL"
  			(at 5.08 3.81 0)
  		)
  		(property "Value" "*"
  			(at 2.286 -3.048 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "8A 250VAC, 6 Poles (5 Form A (NO) + 1 Form B (NC)) Relay With Force Guided Contacts, SR6 Serie"
  			(at 0 0 0)
  		)
  		(symbol "REL_TYCO_SCHRACK_SR6C_1_0"
  			(pin passive line
  				(at 0 0 0)
  				(length 3.81)
  				(name "A1")
  				(number "A1")
  			)
  			(pin passive line
  				(at 10.16 0 180)
  				(length 3.81)
  				(name "A2")
  				(number "A2")
  			)
  		)
  		(symbol "REL_TYCO_SCHRACK_SR6C_2_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "13")
  			)
  			(pin bidirectional line
  				(at 15.24 0 180)
  				(length 4.445)
  				(name "NO")
  				(number "14")
  			)
  		)
  		(symbol "REL_TYCO_SCHRACK_SR6C_3_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "22")
  			)
  			(pin bidirectional line
  				(at 15.24 0 180)
  				(length 4.445)
  				(name "NC")
  				(number "21")
  			)
  		)
  		(symbol "REL_TYCO_SCHRACK_SR6C_4_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "34")
  			)
  			(pin bidirectional line
  				(at 15.24 0 180)
  				(length 4.445)
  				(name "NO")
  				(number "33")
  			)
  		)
  		(symbol "REL_TYCO_SCHRACK_SR6C_5_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "44")
  			)
  			(pin bidirectional line
  				(at 15.24 0 180)
  				(length 4.445)
  				(name "NO")
  				(number "43")
  			)
  		)
  		(symbol "REL_TYCO_SCHRACK_SR6C_6_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "54")
  			)
  			(pin bidirectional line
  				(at 15.24 0 180)
  				(length 4.445)
  				(name "NO")
  				(number "53")
  			)
  		)
  		(symbol "REL_TYCO_SCHRACK_SR6C_7_0"
  			(pin bidirectional line
  				(at 0 0 0)
  				(length 4.445)
  				(name "C")
  				(number "64")
  			)
  			(pin bidirectional line
  				(at 15.24 0 180)
  				(length 4.445)
  				(name "NO")
  				(number "63")
  			)
  		)
  		(embedded_fonts no)
  	)
)
