(footprint "RELS_FINDER_93.11"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Graphical Model for Relay Socket, FINDER_93.11 Series (Do Not Use Alone, Use Only With Relay)")
	(property "Reference" "REF**"
		(at 1.13466 -3.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "RELS_FINDER_93.11"
		(at 1.13466 3.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "13"
		(at 6.4 1.32446 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "A1"
		(at -9.8 1.32446 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "A2"
		(at -13.7 1.32446 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Must be Used with FINDER 34.81 Relay"
		(at -13.36 2.716375 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "12"
		(at 1.4 1.32446 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "14"
		(at 11.3 1.22446 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(pad "12" thru_hole circle
		(at 2.1 -1.2)
		(size 2 2)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "A1" smd circle
		(at -9.15 -1.2)
		(size 1.3 1.3)
		(layers "F.Cu" "F.Paste")
		(solder_mask_margin -0.76)
		(solder_paste_margin -0.66)
		(thermal_bridge_angle 90)
	)
	(pad "A2" smd circle
		(at -12.9 -1.2)
		(size 1.3 1.3)
		(layers "F.Cu" "F.Paste")
		(solder_mask_margin -0.66)
		(solder_paste_margin -0.66)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
