(footprint "RELS_FINDER_94.12"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Graphical Model for Relay Socket, FINDER_94.12 Series (Do Not Use Alone, Use Only With Relay)")
	(property "Reference" "REF**"
		(at 0 -15.55001 0)
		(layer "F.SilkS")
	)
	(property "Value" "RELS_FINDER_94.12"
		(at 0 15.55001 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "11"
		(at 9.53375 1.7 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Must be Used with FINDER 55.32 Relay"
		(at 2.656375 12.7 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "12"
		(at 9.53375 -8.45 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "4"
		(at -3.66625 -8.95001 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "1"
		(at 5.53375 -9.2 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "14"
		(at -3.66625 8.25 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "8"
		(at -3.66625 -4.85 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "A1"
		(at 9.53374 8.25 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "9"
		(at 5.53375 1.45 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "41"
		(at -7.66626 1.95 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "13"
		(at 5.53374 8.25 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "42"
		(at -7.66626 -8.2 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "5"
		(at 5.53375 -4.85 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "A2"
		(at -7.66626 8.50001 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "14"
		(at 9.53375 -4.35 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "44"
		(at -7.66626 -4.1 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "12"
		(at -3.66625 1.95 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(pad "13" smd circle
		(at 6.60001 7.25)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Paste")
		(solder_mask_margin -0.76)
		(solder_paste_margin -0.76)
		(thermal_bridge_angle 90)
	)
	(pad "14" smd circle
		(at -6.60001 7.25)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Paste")
		(solder_mask_margin -0.76)
		(solder_paste_margin -0.76)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
