(footprint "RELS_FINDER_94.14SMA"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Graphical Model for Relay Socket, FINDER_94.14 Series (Do Not Use Alone, Use Only With Relay)")
	(property "Reference" "REF**"
		(at 0 -15.55001 0)
		(layer "F.SilkS")
	)
	(property "Value" "RELS_FINDER_94.14SMA"
		(at 0 15.55001 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "Must be Used with"
		(at -6.5 3.916375 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "12"
		(at -7.66626 1.95 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "8"
		(at -7.71625 -4.8 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "3"
		(at -3.31625 -8.9 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "1"
		(at 5.48376 -8.9 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "11"
		(at -3.31625 1.5 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "14"
		(at -7.71625 8.55001 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "5"
		(at 5.48376 -4.8 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "4"
		(at -7.71625 -8.8 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "FINDER 55.32 Relay"
		(at -6.55 5.649785 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "2"
		(at 1.08376 -8.9 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "7"
		(at -3.31625 -4.8 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "9"
		(at 5.48376 1.5 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "13"
		(at 5.48376 8.55001 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "10"
		(at 1.08375 2 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "6"
		(at 1.08376 -4.8 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(pad "13" smd circle
		(at 6.60001 7.25)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Paste")
		(solder_mask_margin -0.76)
		(solder_paste_margin -0.76)
		(thermal_bridge_angle 90)
	)
	(pad "14" smd circle
		(at -6.60001 7.25)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Paste")
		(solder_mask_margin -0.76)
		(solder_paste_margin -0.76)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
