(footprint "RELS_FINDER_96.12"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Graphical Model for Relay Socket, FINDER_96.12 Series (Do Not Use Alone, Use Only With Relay)")
	(property "Reference" "REF**"
		(at 0 -15.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "RELS_FINDER_96.12"
		(at 0 15.55 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "A2"
		(at -9.75 11.10575 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "2"
		(at -7 -11.41625 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "12"
		(at 8.3 -8.01625 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "5"
		(at 3 -0.81625 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "14"
		(at 8.3 -3.91625 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "8"
		(at -5.6 8.05775 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Must be Used with FINDER 56.32 Relay"
		(at 1.656375 12.7 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "4"
		(at -7 -6.71625 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "41"
		(at -9.75 1.68375 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "11"
		(at 8.3 2.13375 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "6"
		(at -7 -0.81625 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "A1"
		(at 8.3 11.10575 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "42"
		(at -9.75 -8.91625 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "3"
		(at 3 -6.71625 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "7"
		(at 4.191 8.05775 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "44"
		(at -9.75 -3.91625 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "1"
		(at 3 -11.41625 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(pad "A1" smd circle
		(at 8.3 7.3)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Paste")
		(solder_mask_margin -0.76)
		(solder_paste_margin -0.76)
		(thermal_bridge_angle 90)
	)
	(pad "A2" smd circle
		(at -8.3 7.3)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Paste")
		(solder_mask_margin -0.76)
		(solder_paste_margin -0.76)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
