(footprint "RELS_FINDER_97.12"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Relay Socket (No Pin), FINDER_97.12 Series (Do Not Use Alone, Use Only With Relay)")
	(property "Reference" "REF**"
		(at -1.15 -7.01759 0)
		(layer "F.SilkS")
	)
	(property "Value" "RELS_FINDER_97.12"
		(at -1.15 7.01762 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "A1" smd circle
		(at -12.45 3.75 270)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Paste")
		(solder_mask_margin -0.76)
		(solder_paste_margin -0.76)
		(thermal_bridge_angle 90)
	)
	(pad "A2" smd circle
		(at -12.45 -3.75 270)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Paste")
		(solder_mask_margin -0.76)
		(solder_paste_margin -0.76)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
