(footprint "RELS_PANASONIC_SFS4-PS"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "10 Leads Relay Socket, Row Spacing 10.16mm; Body 50mm x 15mm, PANASONIC_SF Series")
	(property "Reference" "REF**"
		(at -0.1 -8.29998 0)
		(layer "F.SilkS")
	)
	(property "Value" "RELS_PANASONIC_SFS4-PS"
		(at -0.1 8.30002 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "1"
		(at -18.3 3.7225 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "4"
		(at 0.5 3.7225 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "5"
		(at -4.53 -2.4775 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "8"
		(at 17.1 3.7225 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "10"
		(at 16.7 -2.4775 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "7"
		(at 12 3.7225 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "6"
		(at 0.55 -2.4775 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "3"
		(at -4.5 3.7225 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "2"
		(at -18.5 -2.4775 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "9"
		(at 11.98 -2.4775 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(pad "" np_thru_hole circle
		(at -22.27 0.00002)
		(size 0.5 0.5)
		(drill 3.2)
		(layers "F&B.Cu" "*.Mask")
		(solder_mask_margin 1.35)
		(thermal_bridge_angle 90)
	)
	(pad "" np_thru_hole circle
		(at 6.63 0.00002)
		(size 0.5 0.5)
		(drill 3.2)
		(layers "F&B.Cu" "*.Mask")
		(solder_mask_margin 1.35)
		(thermal_bridge_angle 90)
	)
	(pad "" np_thru_hole circle
		(at 21.73 0.00002)
		(size 0.5 0.5)
		(drill 3.2)
		(layers "F&B.Cu" "*.Mask")
		(solder_mask_margin 1.35)
		(thermal_bridge_angle 90)
	)
	(pad "1" thru_hole circle
		(at -18.17 5.07998 90)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -18.17 -5.07998 90)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at -4.2 5.07998 90)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at 0.88 5.07998 90)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -4.2 -5.07998 90)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at 0.88 -5.07998)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at 12.31 5.07998)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at 17.39 5.07998)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "9" thru_hole circle
		(at 12.31 -5.07998)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "10" thru_hole circle
		(at 17.39 -5.07998)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
