(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "RELS_TYCO_27E046 [alt]"
  		(pin_names
  			(offset 1.27)
  			(hide yes)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "RLS"
  			(at 5.08 1.524 0)
  		)
  		(property "Value" "*"
  			(at 7.62 -39.37 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "PCB Socket for PANASONIC SFS Relays, 4 Poles"
  			(at 0 0 0)
  		)
  		(symbol "RELS_TYCO_27E046 [alt]_1_0"
  			(text "+"
  				(at 15.24 -2.54 0)
  			)
  			(pin passive line
  				(at 0 -5.08 0)
  				(length 6.35)
  				(name "2")
  				(number "2")
  			)
  			(pin bidirectional line
  				(at 0 -12.7 0)
  				(length 4.445)
  				(name "3")
  				(number "3")
  			)
  			(pin bidirectional line
  				(at 0 -20.32 0)
  				(length 4.445)
  				(name "5")
  				(number "5")
  			)
  			(pin bidirectional line
  				(at 0 -27.94 0)
  				(length 4.445)
  				(name "7")
  				(number "7")
  			)
  			(pin bidirectional line
  				(at 0 -35.56 0)
  				(length 4.445)
  				(name "9")
  				(number "9")
  			)
  			(pin passive line
  				(at 15.24 -5.08 180)
  				(length 6.35)
  				(name "1")
  				(number "1")
  			)
  			(pin bidirectional line
  				(at 15.24 -12.7 180)
  				(length 4.445)
  				(name "4")
  				(number "4")
  			)
  			(pin bidirectional line
  				(at 15.24 -20.32 180)
  				(length 4.445)
  				(name "6")
  				(number "6")
  			)
  			(pin bidirectional line
  				(at 15.24 -27.94 180)
  				(length 4.445)
  				(name "8")
  				(number "8")
  			)
  			(pin bidirectional line
  				(at 15.24 -35.56 180)
  				(length 4.445)
  				(name "10")
  				(number "10")
  			)
  		)
  		(embedded_fonts no)
  	)
)
