(footprint "RELS_TYCO_27E129"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "16 Contacts PCB Socket For TYCO R10 Series Relays")
	(property "Reference" "REF**"
		(at -0.381 -16.92901 0)
		(layer "F.SilkS")
	)
	(property "Value" "RELS_TYCO_27E129"
		(at -0.381 14.74461 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "10"
		(at -6.5313 -10.80751 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5"
		(at -5.36181 -3.1875 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "13"
		(at 3.60839 -5.7275 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "8"
		(at -5.3411 -8.2675 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "3"
		(at 1.15329 10.24911 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "7"
		(at -6.2809 -5.7275 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "2"
		(at -2.65334 11.18891 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at -6.34601 10.24911 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "12"
		(at -0.54113 -3.1875 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at -1.19578 -5.7275 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "15"
		(at -0.53181 -8.2675 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "9"
		(at -1.21773 -10.80751 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "16"
		(at 3.6043 -10.80751 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "11"
		(at 4.6689 -3.1875 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "4"
		(at 4.934 11.18891 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "14"
		(at 4.5189 -8.2675 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -6.0325 11.43001)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at -2.2225 8.89001)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 1.5875 11.43001)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at 5.3975 8.89001)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -6.6675 -3.81)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at 0.9525 -6.35)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at -4.1275 -6.35)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "8" thru_hole circle
		(at -6.6675 -8.89001)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "9" thru_hole circle
		(at 0.9525 -11.43001)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "10" thru_hole circle
		(at -4.1275 -11.43001)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "11" thru_hole circle
		(at 3.4925 -3.81)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "12" thru_hole circle
		(at -1.5875 -3.81)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "13" thru_hole circle
		(at 6.0325 -6.35)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "14" thru_hole circle
		(at 3.4925 -8.89001)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "15" thru_hole circle
		(at -1.5875 -8.89001)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "16" thru_hole circle
		(at 6.0325 -11.43001)
		(size 2.1 2.1)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
