(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ADXL362BCCZ-RL7"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ADXL362BCCZ-RL7"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ADXL362BCCZ-RL7"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/609/adxl362-3122260.pdf"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Digital Accelerometer, Nanopower Three-Axis, 2g/4g/8g"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ADXL362BCCZ-RL7"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IMU, MEMS, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "InvenSense?QFN*3x3mm*P0.4mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ADXL362BCCZ-RL7_1_1"
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "V_{DDIO}")
					(number "1")
				)
				(pin no_connect line
					(at 20.32 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "2")
				)
				(pin no_connect line
					(at 20.32 -7.62 180)
					(length 2.54)
					(hide yes)
					(name "RESERVED")
					(number "3")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "SCLK")
					(number "4")
				)
				(pin no_connect line
					(at 20.32 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "RESERVED")
					(number "5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "MOSI")
					(number "6")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 2.54)
					(name "MISO")
					(number "7")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{CS}")
					(number "8")
				)
				(pin bidirectional line
					(at 22.86 -2.54 180)
					(length 2.54)
					(name "INT2")
					(number "9")
				)
				(pin no_connect line
					(at 20.32 -10.16 180)
					(length 2.54)
					(hide yes)
					(name "RESERVED")
					(number "10")
				)
				(pin bidirectional line
					(at 22.86 0 180)
					(length 2.54)
					(name "INT1")
					(number "11")
				)
				(pin passive line
					(at 22.86 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "12")
				)
				(pin passive line
					(at 22.86 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "13")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{S}")
					(number "14")
				)
				(pin no_connect line
					(at 20.32 -6.35 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "15")
				)
				(pin passive line
					(at 22.86 -12.7 180)
					(length 2.54)
					(name "GND")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
