(footprint "BGA-25-24_6x8mm_Layout5x5_P1x1mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -4.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-25-24_6x8mm_Layout5x5_P1x1mm"
		(at 0 5.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -3.25 8.332 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -3.25 9.532 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -3.25 10.732 0)
		(layer "F.Fab")
	)
	(pad "A2" smd circle
		(at -1 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "A3" smd circle
		(at 0 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "A4" smd circle
		(at 1 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "A5" smd circle
		(at 2 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "B1" smd circle
		(at -2 -1)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "B2" smd circle
		(at -1 -1)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "B3" smd circle
		(at 0 -1)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "B4" smd circle
		(at 1 -1)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "B5" smd circle
		(at 2 -1)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "C1" smd circle
		(at -2 0)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "C2" smd circle
		(at -1 0)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "C3" smd circle
		(at 0 0)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "C4" smd circle
		(at 1 0)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "C5" smd circle
		(at 2 0)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "D1" smd circle
		(at -2 1)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "D2" smd circle
		(at -1 1)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "D3" smd circle
		(at 0 1)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "D4" smd circle
		(at 1 1)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "D5" smd circle
		(at 2 1)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "E1" smd circle
		(at -2 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "E2" smd circle
		(at -1 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "E3" smd circle
		(at 0 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "E4" smd circle
		(at 1 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(pad "E5" smd circle
		(at 2 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.102)
	)
	(embedded_fonts no)
	(model "antmicro_aps256xxn_obr_wa.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
