(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "APS256XXN-OBR-WA"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "APS256XXN-OBR-WA"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "APS256XXN-OBR-WA"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.apmemory.com/wp-content/uploads/APM_PSRAM_OPI_Xccela-APS256XXN-OBRx-v1.0-PKG.pdf"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DRAM RAM 256Mb OPI (x8,x16) DDR 200MHz, 1.8V, Industrial Grade Temperature"
				(at 33.02 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "APS256XXN-OBR-WA"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "AP Memory"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MEMORY, DRAM, BGA, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "APS256XXN-OBR-WA_1_1"
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "DQ10")
					(number "A2")
				)
				(pin passive line
					(at 19.05 -2.54 180)
					(length 2.54)
					(name "~{CE}")
					(number "A3")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "DQ11")
					(number "A4")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "DQ12")
					(number "A5")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "DQ9")
					(number "B1")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "CLK")
					(number "B2")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "DQS/DM1")
					(number "B3")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "DQ13")
					(number "B4")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "DQ14")
					(number "B5")
				)
				(pin power_in line
					(at 19.05 -45.72 180)
					(length 2.54)
					(name "VSS")
					(number "C1")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "DQ8")
					(number "C2")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "DQS/DM0")
					(number "C3")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "ADQ2")
					(number "C4")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "DQ15")
					(number "C5")
				)
				(pin power_in line
					(at 19.05 0 180)
					(length 2.54)
					(name "VDD")
					(number "D1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "ADQ1")
					(number "D2")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "ADQ0")
					(number "D3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "ADQ3")
					(number "D4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "ADQ4")
					(number "D5")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "ADQ7")
					(number "E1")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "ADQ6")
					(number "E2")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "ADQ5")
					(number "E3")
				)
				(pin passive line
					(at 19.05 0 180)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "E4")
				)
				(pin passive line
					(at 19.05 -45.72 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "E5")
				)
			)
			(embedded_fonts no)
		)
)
