(footprint "Bosch_WLCSP-6_0.84x1.18mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -0.67 -1.39 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Bosch_WLCSP-6_0.84x1.18mm"
		(at -0.67 1.94 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at -0.65 6.7 0)
		(layer "F.Fab")
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -0.67 3.14 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -0.67 4.34 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -0.67 5.54 0)
		(layer "F.Fab")
	)
	(fp_text user ""
		(at 0 0 0)
		(layer "User.5")
	)
	(pad "1" smd circle
		(at -0.2 -0.4)
		(size 0.18 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.04)
	)
	(pad "2" smd circle
		(at -0.2 0)
		(size 0.18 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.04)
	)
	(pad "3" smd circle
		(at -0.2 0.4)
		(size 0.18 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.04)
	)
	(pad "4" smd circle
		(at 0.2 0.4)
		(size 0.18 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.04)
	)
	(pad "5" smd circle
		(at 0.2 0)
		(size 0.18 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.04)
	)
	(pad "6" smd circle
		(at 0.2 -0.4)
		(size 0.18 0.18)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.04)
	)
	(embedded_fonts no)
	(model "antmicro_bma580.glb"
		(offset
			(xyz -0 -0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
