(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "BMA580"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "BMA580"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "BMA580"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.bosch-sensortec.com/media/boschsensortec/downloads/datasheets/bst-bma580-ds000.pdf"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "SPI/I2C/I3C, 3-axis Accelerometer, BGA 6-WLCSP, VDD 1.6V - 3.6V"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Bosch"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "BMA580"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "BGA, SENSOR, IC, I2C, I3C, SPI"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "BMA580_1_1"
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "VSS")
					(number "1")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 2.54)
					(name "INT1")
					(number "2")
					(alternate "SDO" output line)
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 2.54)
					(name "INT2")
					(number "3")
					(alternate "CSB" input line)
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SDA")
					(number "4")
					(alternate "SDI" input line)
					(alternate "SDX" bidirectional line)
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SCL")
					(number "5")
					(alternate "SCK" input line)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
