(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "BNO085"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "BNO085"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "BNO085"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ceva-dsp.com/wp-content/uploads/2019/10/BNO080_085-Datasheet.pdf"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Motion sensor (IMU)"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "BNO085"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "CEVA Technologies"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, SENSOR, IC, SOM"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "BNO085_1_1"
				(pin no_connect line
					(at 22.86 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "RESV_NC")
					(number "1")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "3")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 2.54)
					(name "BOOTN")
					(number "4")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "PS1")
					(number "5")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 2.54)
					(name "PS0")
					(number "6")
					(alternate "WAKE" input line)
				)
				(pin no_connect line
					(at 22.86 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "RESV_NC")
					(number "7")
				)
				(pin no_connect line
					(at 22.86 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "RESV_NC")
					(number "8")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 2.54)
					(name "CAP")
					(number "9")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 2.54)
					(name "CLKSEL0")
					(number "10")
				)
				(pin input line
					(at 25.4 -12.7 180)
					(length 2.54)
					(name "NRST")
					(number "11")
				)
				(pin no_connect line
					(at 22.86 -22.86 180)
					(length 2.54)
					(hide yes)
					(name "RESV_NC")
					(number "12")
				)
				(pin no_connect line
					(at 22.86 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "RESV_NC")
					(number "13")
				)
				(pin output line
					(at 0 -13.97 0)
					(length 2.54)
					(name "H_INTN")
					(number "14")
				)
				(pin passive line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "ENV_SCL")
					(number "15")
				)
				(pin passive line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "ENV_SDA")
					(number "16")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "SA0")
					(number "17")
					(alternate "H_MOSI" input line)
				)
				(pin input line
					(at 0 -26.67 0)
					(length 2.54)
					(name "H_CSN")
					(number "18")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "H_SCL")
					(number "19")
					(alternate "RX" input line)
					(alternate "SCK" input line)
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "H_SDA")
					(number "20")
					(alternate "H_MISO" bidirectional line)
					(alternate "TX" output line)
				)
				(pin no_connect line
					(at 22.86 -27.94 180)
					(length 2.54)
					(hide yes)
					(name "RESV_NC")
					(number "21")
				)
				(pin no_connect line
					(at 22.86 -30.48 180)
					(length 2.54)
					(hide yes)
					(name "RESV_NC")
					(number "22")
				)
				(pin no_connect line
					(at 10.795 -33.02 90)
					(length 2.54)
					(hide yes)
					(name "RESV_NC")
					(number "23")
				)
				(pin no_connect line
					(at 8.255 -33.02 90)
					(length 2.54)
					(hide yes)
					(name "RESV_NC")
					(number "24")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "25")
				)
				(pin output line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "XOUT32")
					(number "26")
					(alternate "CLKSEL1" output line)
				)
				(pin input line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "XIN32")
					(number "27")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDDIO")
					(number "28")
				)
			)
			(embedded_fonts no)
		)
)
