(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ICM-40609-D"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ICM-40609-D"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ICM-40609-D"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://product.tdk.com/system/files/dam/doc/product/sensor/mortion-inertial/imu/data_sheet/ds-000330_icm-40609-d_v1.2.pdf"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "High precision Inertial Measurement Unit device for Drone market with accelerometer, gyroscope, 6 axis sensor, MEMS, MotionTracking, I2C, SPI output"
				(at 38.1 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ICM-40609-D"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "TDK"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IMU, MEMS, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ICM-40609-D_1_1"
				(pin no_connect line
					(at 2.54 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "1")
				)
				(pin no_connect line
					(at 2.54 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "2")
				)
				(pin no_connect line
					(at 2.54 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "3")
				)
				(pin no_connect line
					(at 2.54 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "4")
				)
				(pin no_connect line
					(at 2.54 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin no_connect line
					(at 2.54 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "6")
				)
				(pin no_connect line
					(at 2.54 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "7")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDDIO")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "AD0")
					(number "9")
					(alternate "SDO" passive line)
				)
				(pin no_connect line
					(at 2.54 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "RESV")
					(number "11")
				)
				(pin output line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "INT1")
					(number "12")
					(alternate "INT" passive line)
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "13")
				)
				(pin no_connect line
					(at 2.54 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "14")
				)
				(pin no_connect line
					(at 2.54 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "15")
				)
				(pin no_connect line
					(at 2.54 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "16")
				)
				(pin no_connect line
					(at 2.54 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "17")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 2.54)
					(name "GND")
					(number "18")
				)
				(pin bidirectional line
					(at 25.4 0 180)
					(length 2.54)
					(name "INT2")
					(number "19")
					(alternate "FSYNC" passive line)
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "RESV")
					(number "20")
				)
				(pin no_connect line
					(at 2.54 -22.86 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "21")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{CS}")
					(number "22")
				)
				(pin input clock
					(at 0 -5.08 0)
					(length 2.54)
					(name "SCL")
					(number "23")
					(alternate "SCLK" passive line)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SDA")
					(number "24")
					(alternate "SDI" passive line)
					(alternate "SDIO" passive line)
				)
			)
			(embedded_fonts no)
		)
)
