(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ICM-42605"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ICM-42605"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ICM-42605"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://invensense.tdk.com/wp-content/uploads/2022/09/DS-000292-ICM-42605-v1.7.pdf"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Motion sensor (IMU)"
				(at 38.1 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "TDK"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ICM-42605"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, IMU, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "InvenSense?QFN*3x3mm*P0.4mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ICM-42605_1_1"
				(pin output line
					(at 0 -7.62 0)
					(length 2.54)
					(name "AD0/SDO")
					(number "1")
				)
				(pin no_connect line
					(at 22.86 -7.62 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "2")
				)
				(pin no_connect line
					(at 22.86 -10.16 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "3")
				)
				(pin output line
					(at 0 -22.86 0)
					(length 2.54)
					(name "INT")
					(number "4")
				)
				(pin power_in line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "VDDIO")
					(number "5")
				)
				(pin power_in line
					(at 25.4 -22.86 180)
					(length 2.54)
					(name "GND")
					(number "6")
				)
				(pin no_connect line
					(at 22.86 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "7")
				)
				(pin power_in line
					(at 25.4 0 180)
					(length 2.54)
					(name "VDD")
					(number "8")
				)
				(pin output line
					(at 0 -20.32 0)
					(length 2.54)
					(name "FSYNC/INT2")
					(number "9")
				)
				(pin no_connect line
					(at 22.86 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "10")
				)
				(pin no_connect line
					(at 22.86 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "11")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "CS")
					(number "12")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "SCL/SCLK")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SDA/SDIO")
					(number "14")
				)
			)
			(embedded_fonts no)
		)
)
